# Static Call Graph for image .\Objects\SX126xSTM32F103C8Demo.axf

#<CALLGRAPH># ARM Linker, 5060750: Last Updated: Wed Aug 24 15:32:29 2022

### Maximum Stack Usage = 360 bytes + Unknown(Functions without stacksize, Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

RadioIsChannelFree ⇒ RadioSetRxConfig ⇒ SX126xSetPacketParams ⇒ SX126xSetCrcSeed ⇒ SX126xWriteRegisters ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf

### Functions with no stack information

- __user_initial_stackheap

### Mutually Recursive functions

- ADC1_2_IRQHandler ⇒ ADC1_2_IRQHandler
- RadioSetPublicNetwork ⇒ RadioSetModem

  ### Function Pointers

  - ADC1_2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - ADC3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - BusFault_Handler from stm32f10x_it.o(i.BusFault_Handler) referenced from startup_stm32f10x_hd.o(RESET)
  - CAN1_RX1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - CAN1_SCE_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel4_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel6_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel7_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel4_5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DebugMon_Handler from stm32f10x_it.o(i.DebugMon_Handler) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI0_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI15_10_IRQHandler from sx126xstm32f103-board.o(i.EXTI15_10_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI4_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI9_5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - FLASH_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - FSMC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - HardFault_Handler from stm32f10x_it.o(i.HardFault_Handler) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - MemManage_Handler from stm32f10x_it.o(i.MemManage_Handler) referenced from startup_stm32f10x_hd.o(RESET)
  - NMI_Handler from stm32f10x_it.o(i.NMI_Handler) referenced from startup_stm32f10x_hd.o(RESET)
  - PVD_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - PendSV_Handler from stm32f10x_it.o(i.PendSV_Handler) referenced from startup_stm32f10x_hd.o(RESET)
  - RCC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - RTCAlarm_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - RTC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - RadioCheckRfFrequency from radio.o(i.RadioCheckRfFrequency) referenced from radio.o(.constdata)
  - RadioGetStatus from radio.o(i.RadioGetStatus) referenced from radio.o(.constdata)
  - RadioGetWakeupTime from radio.o(i.RadioGetWakeupTime) referenced from radio.o(.constdata)
  - RadioInit from radio.o(i.RadioInit) referenced from radio.o(.constdata)
  - RadioIrqProcess from radio.o(i.RadioIrqProcess) referenced from radio.o(.constdata)
  - RadioIsChannelFree from radio.o(i.RadioIsChannelFree) referenced from radio.o(.constdata)
  - RadioOnDioIrq from radio.o(i.RadioOnDioIrq) referenced from radio.o(i.RadioInit)
  - RadioRandom from radio.o(i.RadioRandom) referenced from radio.o(.constdata)
  - RadioRead from radio.o(i.RadioRead) referenced from radio.o(.constdata)
  - RadioReadBuffer from radio.o(i.RadioReadBuffer) referenced from radio.o(.constdata)
  - RadioRssi from radio.o(i.RadioRssi) referenced from radio.o(.constdata)
  - RadioRx from radio.o(i.RadioRx) referenced from radio.o(.constdata)
  - RadioRxBoosted from radio.o(i.RadioRxBoosted) referenced from radio.o(.constdata)
  - RadioSend from radio.o(i.RadioSend) referenced from radio.o(.constdata)
  - RadioSetChannel from radio.o(i.RadioSetChannel) referenced from radio.o(.constdata)
  - RadioSetMaxPayloadLength from radio.o(i.RadioSetMaxPayloadLength) referenced from radio.o(.constdata)
  - RadioSetModem from radio.o(i.RadioSetModem) referenced from radio.o(.constdata)
  - RadioSetPublicNetwork from radio.o(i.RadioSetPublicNetwork) referenced from radio.o(.constdata)
  - RadioSetRxConfig from radio.o(i.RadioSetRxConfig) referenced from radio.o(.constdata)
  - RadioSetRxDutyCycle from radio.o(i.RadioSetRxDutyCycle) referenced from radio.o(.constdata)
  - RadioSetTxConfig from radio.o(i.RadioSetTxConfig) referenced from radio.o(.constdata)
  - RadioSetTxContinuousWave from radio.o(i.RadioSetTxContinuousWave) referenced from radio.o(.constdata)
  - RadioSleep from radio.o(i.RadioSleep) referenced from radio.o(.constdata)
  - RadioStandby from radio.o(i.RadioStandby) referenced from radio.o(.constdata)
  - RadioStartCad from radio.o(i.RadioStartCad) referenced from radio.o(.constdata)
  - RadioTimeOnAir from radio.o(i.RadioTimeOnAir) referenced from radio.o(.constdata)
  - RadioWrite from radio.o(i.RadioWrite) referenced from radio.o(.constdata)
  - RadioWriteBuffer from radio.o(i.RadioWriteBuffer) referenced from radio.o(.constdata)
  - Reset_Handler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SDIO_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SPI1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SPI2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SPI3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SVC_Handler from stm32f10x_it.o(i.SVC_Handler) referenced from startup_stm32f10x_hd.o(RESET)
  - SX126xOnRxDone from sx126x_example_send.o(i.SX126xOnRxDone) referenced from sx126x_example_send.o(i.ExampleSX126xSendDemo)
  - SX126xOnRxError from sx126x_example_send.o(i.SX126xOnRxError) referenced from sx126x_example_send.o(i.ExampleSX126xSendDemo)
  - SX126xOnRxTimeout from sx126x_example_send.o(i.SX126xOnRxTimeout) referenced from sx126x_example_send.o(i.ExampleSX126xSendDemo)
  - SX126xOnTxDone from sx126x_example_send.o(i.SX126xOnTxDone) referenced from sx126x_example_send.o(i.ExampleSX126xSendDemo)
  - SX126xOnTxTimeout from sx126x_example_send.o(i.SX126xOnTxTimeout) referenced from sx126x_example_send.o(i.ExampleSX126xSendDemo)
  - SysTick_Handler from stm32f10x_it.o(i.SysTick_Handler) referenced from startup_stm32f10x_hd.o(RESET)
  - SystemInit from system_stm32f10x.o(i.SystemInit) referenced from startup_stm32f10x_hd.o(.text)
  - TAMPER_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_BRK_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_TRG_COM_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_UP_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM3_IRQHandler from sx126xstm32f103-board.o(i.TIM3_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM4_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM6_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM7_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_BRK_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_CC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_TRG_COM_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_UP_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - UART4_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - UART5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USART1_IRQHandler from hal_uart.o(i.USART1_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - USART2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USART3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USBWakeUp_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USB_HP_CAN1_TX_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USB_LP_CAN1_RX0_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - UsageFault_Handler from stm32f10x_it.o(i.UsageFault_Handler) referenced from startup_stm32f10x_hd.o(RESET)
  - WWDG_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - __main from __main.o(!!!main) referenced from startup_stm32f10x_hd.o(.text)
  - _printf_input_char from _printf_char_common.o(.text) referenced from _printf_char_common.o(.text)
  - fputc from hal_uart.o(i.fputc) referenced from _printf_char_file.o(.text)

  ### Global Symbols

  __main (Thumb, 8 bytes, Stack size 0 bytes, __main.o(!!!main))
  [Calls]

  - >> __scatterload
  - >> __rt_entry

  __scatterload (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter))
  [Called By]

  - >> __main

  __scatterload_rt2 (Thumb, 44 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)
  [Calls]

  - >> __rt_entry

  __scatterload_rt2_thumb_only (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_null (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_copy (Thumb, 26 bytes, Stack size unknown bytes, __scatter_copy.o(!!handler_copy), UNUSED)
  [Calls]

  - >> __scatterload_copy
  [Called By]
  - >> __scatterload_copy

  __scatterload_zeroinit (Thumb, 28 bytes, Stack size unknown bytes, __scatter_zi.o(!!handler_zi), UNUSED)

  _printf_d (Thumb, 0 bytes, Stack size unknown bytes, _printf_d.o(.ARM.Collect$$_printf_percent$$00000009))
  [Stack]

  - Max Depth = 72 + Unknown Stack Size
  - Call Chain = _printf_d ⇒ _printf_int_dec ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_int_dec

  _printf_percent (Thumb, 0 bytes, Stack size unknown bytes, _printf_percent.o(.ARM.Collect$$_printf_percent$$00000000))
  [Called By]

  - >> __printf

  _printf_x (Thumb, 0 bytes, Stack size unknown bytes, _printf_x.o(.ARM.Collect$$_printf_percent$$0000000C))
  [Stack]

  - Max Depth = 64 + Unknown Stack Size
  - Call Chain = _printf_x ⇒ _printf_int_hex ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_int_hex

  _printf_s (Thumb, 0 bytes, Stack size unknown bytes, _printf_s.o(.ARM.Collect$$_printf_percent$$00000014))
  [Stack]

  - Max Depth = 40 + Unknown Stack Size
  - Call Chain = _printf_s ⇒ _printf_string ⇒ _printf_cs_common ⇒ _printf_str ⇒ _printf_post_padding
  [Calls]
  - >> _printf_string

  _printf_percent_end (Thumb, 0 bytes, Stack size unknown bytes, _printf_percent_end.o(.ARM.Collect$$_printf_percent$$00000017))

  __rt_lib_init (Thumb, 0 bytes, Stack size unknown bytes, libinit.o(.ARM.Collect$$libinit$$00000000))
  [Called By]

  - >> __rt_entry_li

  __rt_lib_init_alloca_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002E))

  __rt_lib_init_argv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002C))

  __rt_lib_init_atexit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001B))

  __rt_lib_init_clock_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000021))

  __rt_lib_init_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000032))

  __rt_lib_init_exceptions_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000030))

  __rt_lib_init_fp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000002))

  __rt_lib_init_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001F))

  __rt_lib_init_getenv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000023))

  __rt_lib_init_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000A))

  __rt_lib_init_lc_collate_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000011))

  __rt_lib_init_lc_ctype_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000013))

  __rt_lib_init_lc_monetary_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000015))

  __rt_lib_init_lc_numeric_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000017))

  __rt_lib_init_lc_time_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000019))

  __rt_lib_init_preinit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000004))

  __rt_lib_init_rand_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000E))

  __rt_lib_init_return (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000033))

  __rt_lib_init_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001D))

  __rt_lib_init_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000025))

  __rt_lib_init_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000C))

  __rt_lib_shutdown (Thumb, 0 bytes, Stack size unknown bytes, libshutdown.o(.ARM.Collect$$libshutdown$$00000000))
  [Called By]

  - >> __rt_exit_ls

  __rt_lib_shutdown_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000002))

  __rt_lib_shutdown_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000007))

  __rt_lib_shutdown_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000F))

  __rt_lib_shutdown_return (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000010))

  __rt_lib_shutdown_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000A))

  __rt_lib_shutdown_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000004))

  __rt_lib_shutdown_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000C))

  __rt_entry (Thumb, 0 bytes, Stack size unknown bytes, __rtentry.o(.ARM.Collect$$rtentry$$00000000))
  [Called By]

  - >> __scatterload_rt2
  - >> __main

  __rt_entry_presh_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$00000002))

  __rt_entry_sh (Thumb, 0 bytes, Stack size unknown bytes, __rtentry4.o(.ARM.Collect$$rtentry$$00000004))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __rt_entry_sh ⇒ __user_setup_stackheap
  [Calls]
  - >> __user_setup_stackheap

  __rt_entry_li (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000A))
  [Calls]

  - >> __rt_lib_init

  __rt_entry_postsh_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$00000009))

  __rt_entry_main (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000D))
  [Stack]

  - Max Depth = 184 + Unknown Stack Size
  - Call Chain = __rt_entry_main ⇒ main ⇒ ExampleSX126xSendDemo ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> main
  - >> exit

  __rt_entry_postli_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000C))

  __rt_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit.o(.ARM.Collect$$rtexit$$00000000))
  [Called By]

  - >> exit

  __rt_exit_ls (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000003))
  [Calls]

  - >> __rt_lib_shutdown

  __rt_exit_prels_1 (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000002))

  __rt_exit_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000004))
  [Calls]

  - >> _sys_exit

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  ADC1_2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Calls]

  - >> ADC1_2_IRQHandler
  [Called By]
  - >> ADC1_2_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  ADC3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel4_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  FSMC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  RTCAlarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  RTC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SDIO_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SPI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TAMPER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  UART4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  UART5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USBWakeUp_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USB_HP_CAN1_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USB_LP_CAN1_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  __user_initial_stackheap (Thumb, 0 bytes, Stack size unknown bytes, startup_stm32f10x_hd.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __use_no_semihosting (Thumb, 2 bytes, Stack size 0 bytes, use_no_semi_2.o(.text), UNUSED)

  __2printf (Thumb, 20 bytes, Stack size 24 bytes, noretval__2printf.o(.text))
  [Stack]

  - Max Depth = 144 + Unknown Stack Size
  - Call Chain = __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> _printf_char_file
  [Called By]
  - >> ExampleSX126xSendDemo
  - >> main
  - >> SX126xWaitOnBusy
  - >> SX126xTxTimerStop
  - >> SX126xTxTimerStart
  - >> SX126xSetTxTimerValue
  - >> SX126xSetRxTimerValue
  - >> SX126xRxTimerStop
  - >> SX126xRxTimerStart
  - >> SX126xIoInit
  - >> EXTI15_10_IRQHandler
  - >> SX126xOnTxTimeout
  - >> SX126xOnTxDone
  - >> SX126xOnRxTimeout
  - >> SX126xOnRxError
  - >> SX126xOnRxDone

  _printf_pre_padding (Thumb, 44 bytes, Stack size 16 bytes, _printf_pad.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = _printf_pre_padding
  [Called By]
  - >> _printf_int_common
  - >> _printf_str

  _printf_post_padding (Thumb, 34 bytes, Stack size 16 bytes, _printf_pad.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = _printf_post_padding
  [Called By]
  - >> _printf_int_common
  - >> _printf_str

  _printf_str (Thumb, 82 bytes, Stack size 16 bytes, _printf_str.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = _printf_str ⇒ _printf_post_padding
  [Calls]
  - >> _printf_post_padding
  - >> _printf_pre_padding
  [Called By]
  - >> _printf_cs_common

  _printf_int_dec (Thumb, 104 bytes, Stack size 24 bytes, _printf_dec.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = _printf_int_dec ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_int_common
  [Called By]
  - >> _printf_d

  _printf_int_hex (Thumb, 84 bytes, Stack size 16 bytes, _printf_hex_int.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = _printf_int_hex ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_int_common
  [Called By]
  - >> _printf_x

  _printf_longlong_hex (Thumb, 0 bytes, Stack size 16 bytes, _printf_hex_int.o(.text), UNUSED)

  __printf (Thumb, 308 bytes, Stack size 40 bytes, __printf_flags_wp.o(.text))
  [Stack]

  - Max Depth = 40 + Unknown Stack Size
  - Call Chain = __printf
  [Calls]
  - >> _printf_percent
  - >> _is_digit
  [Called By]
  - >> _printf_char_common

  __aeabi_memclr4 (Thumb, 0 bytes, Stack size 4 bytes, rt_memclr_w.o(.text))
  [Stack]

  - Max Depth = 4
  - Call Chain = __aeabi_memclr4
  [Called By]
  - >> SX126xGetPacketStatus

  __aeabi_memclr8 (Thumb, 0 bytes, Stack size 4 bytes, rt_memclr_w.o(.text), UNUSED)

  __rt_memclr_w (Thumb, 78 bytes, Stack size 4 bytes, rt_memclr_w.o(.text), UNUSED)

  _memset_w (Thumb, 0 bytes, Stack size unknown bytes, rt_memclr_w.o(.text), UNUSED)

  __use_two_region_memory (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_escrow$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_expand$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __I$use$semihosting (Thumb, 0 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __use_no_semihosting_swi (Thumb, 2 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  _printf_int_common (Thumb, 178 bytes, Stack size 32 bytes, _printf_intcommon.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_post_padding
  - >> _printf_pre_padding
  [Called By]
  - >> _printf_int_hex
  - >> _printf_int_dec

  _printf_cs_common (Thumb, 20 bytes, Stack size 8 bytes, _printf_char.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = _printf_cs_common ⇒ _printf_str ⇒ _printf_post_padding
  [Calls]
  - >> _printf_str
  [Called By]
  - >> _printf_string
  - >> _printf_char

  _printf_char (Thumb, 16 bytes, Stack size 0 bytes, _printf_char.o(.text), UNUSED)
  [Calls]

  - >> _printf_cs_common

  _printf_string (Thumb, 8 bytes, Stack size 0 bytes, _printf_char.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = _printf_string ⇒ _printf_cs_common ⇒ _printf_str ⇒ _printf_post_padding
  [Calls]
  - >> _printf_cs_common
  [Called By]
  - >> _printf_s

  _printf_char_file (Thumb, 32 bytes, Stack size 16 bytes, _printf_char_file.o(.text))
  [Stack]

  - Max Depth = 120 + Unknown Stack Size
  - Call Chain = _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> ferror
  - >> _printf_char_common
  [Called By]
  - >> __2printf

  _printf_char_common (Thumb, 32 bytes, Stack size 64 bytes, _printf_char_common.o(.text))
  [Stack]

  - Max Depth = 104 + Unknown Stack Size
  - Call Chain = _printf_char_common ⇒ __printf
  [Calls]
  - >> __printf
  [Called By]
  - >> _printf_char_file

  ferror (Thumb, 8 bytes, Stack size 0 bytes, ferror.o(.text))
  [Called By]

  - >> _printf_char_file

  __user_setup_stackheap (Thumb, 74 bytes, Stack size 8 bytes, sys_stackheap_outer.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __user_setup_stackheap
  [Calls]
  - >> __user_initial_stackheap
  - >> __user_perproc_libspace
  [Called By]
  - >> __rt_entry_sh

  exit (Thumb, 18 bytes, Stack size 8 bytes, exit.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = exit
  [Calls]
  - >> __rt_exit
  [Called By]
  - >> __rt_entry_main

  __user_libspace (Thumb, 8 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  __user_perproc_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __user_perthread_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  BusFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(i.BusFault_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.DebugMon_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 44 bytes, Stack size 8 bytes, sx126xstm32f103-board.o(i.EXTI15_10_IRQHandler))
  [Stack]

  - Max Depth = 152 + Unknown Stack Size
  - Call Chain = EXTI15_10_IRQHandler ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> GPIO_ReadInputDataBit
  - >> EXTI_ClearITPendingBit
  - >> __2printf
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  EXTI_ClearITPendingBit (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_exti.o(i.EXTI_ClearITPendingBit))
  [Called By]

  - >> SX126xIoIrqInit
  - >> EXTI15_10_IRQHandler

  EXTI_Init (Thumb, 142 bytes, Stack size 0 bytes, stm32f10x_exti.o(i.EXTI_Init))
  [Called By]

  - >> SX126xIoIrqInit

  ExampleSX126xSendDemo (Thumb, 212 bytes, Stack size 40 bytes, sx126x_example_send.o(i.ExampleSX126xSendDemo))
  [Stack]

  - Max Depth = 184 + Unknown Stack Size
  - Call Chain = ExampleSX126xSendDemo ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> delay_ms
  - >> __2printf
  [Called By]
  - >> main

  GPIO_EXTILineConfig (Thumb, 60 bytes, Stack size 12 bytes, stm32f10x_gpio.o(i.GPIO_EXTILineConfig))
  [Stack]

  - Max Depth = 12
  - Call Chain = GPIO_EXTILineConfig
  [Called By]
  - >> SX126xIoIrqInit

  GPIO_Init (Thumb, 278 bytes, Stack size 24 bytes, stm32f10x_gpio.o(i.GPIO_Init))
  [Stack]

  - Max Depth = 24
  - Call Chain = GPIO_Init
  [Called By]
  - >> HALUart1Init
  - >> SysInit
  - >> Spi1Init
  - >> SX126xReset
  - >> SX126xIoIrqInit
  - >> SX126xIoInit

  GPIO_PinRemapConfig (Thumb, 138 bytes, Stack size 20 bytes, stm32f10x_gpio.o(i.GPIO_PinRemapConfig))
  [Stack]

  - Max Depth = 20
  - Call Chain = GPIO_PinRemapConfig
  [Called By]
  - >> SysInit

  GPIO_ReadInputDataBit (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_gpio.o(i.GPIO_ReadInputDataBit))
  [Called By]

  - >> SX126xWaitOnBusy
  - >> EXTI15_10_IRQHandler

  GPIO_ResetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_gpio.o(i.GPIO_ResetBits))
  [Called By]

  - >> main
  - >> SX126xSetNss

  GPIO_SetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_gpio.o(i.GPIO_SetBits))
  [Called By]

  - >> main
  - >> SysInit
  - >> Spi1Init
  - >> SX126xSetNss

  GPIO_WriteBit (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_gpio.o(i.GPIO_WriteBit))
  [Called By]

  - >> SX126xReset

  Get_SysTick (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_it.o(i.Get_SysTick))
  [Called By]

  - >> main

  HALSpi1InOut (Thumb, 82 bytes, Stack size 16 bytes, hal_spi.o(i.HALSpi1InOut))
  [Stack]

  - Max Depth = 16
  - Call Chain = HALSpi1InOut
  [Calls]
  - >> SPI_I2S_SendData
  - >> SPI_I2S_ReceiveData
  - >> SPI_I2S_GetFlagStatus
  [Called By]
  - >> SX126xSpiInOut

  HALUart1Init (Thumb, 162 bytes, Stack size 32 bytes, hal_uart.o(i.HALUart1Init))
  [Stack]

  - Max Depth = 100
  - Call Chain = HALUart1Init ⇒ USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> NVIC_Init
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_Init
  - >> USART_Init
  - >> USART_ITConfig
  - >> USART_DeInit
  - >> USART_Cmd
  [Called By]
  - >> SysInit

  HardFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(i.HardFault_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  MemManage_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(i.MemManage_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.NMI_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  NVIC_Init (Thumb, 100 bytes, Stack size 16 bytes, misc.o(i.NVIC_Init))
  [Stack]

  - Max Depth = 16
  - Call Chain = NVIC_Init
  [Called By]
  - >> HALUart1Init
  - >> SX126xTimerInit
  - >> SX126xIoIrqInit

  NVIC_PriorityGroupConfig (Thumb, 10 bytes, Stack size 0 bytes, misc.o(i.NVIC_PriorityGroupConfig))
  [Called By]

  - >> SysInit

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.PendSV_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  RCC_APB1PeriphClockCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_APB1PeriphClockCmd))
  [Called By]

  - >> SX126xTimerInit

  RCC_APB1PeriphResetCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_APB1PeriphResetCmd))
  [Called By]

  - >> USART_DeInit

  RCC_APB2PeriphClockCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_APB2PeriphClockCmd))
  [Called By]

  - >> HALUart1Init
  - >> SysInit
  - >> Spi1Init
  - >> SX126xReset
  - >> SX126xIoIrqInit
  - >> SX126xIoInit

  RCC_APB2PeriphResetCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_APB2PeriphResetCmd))
  [Called By]

  - >> USART_DeInit

  RCC_GetClocksFreq (Thumb, 192 bytes, Stack size 12 bytes, stm32f10x_rcc.o(i.RCC_GetClocksFreq))
  [Stack]

  - Max Depth = 12
  - Call Chain = RCC_GetClocksFreq
  [Called By]
  - >> USART_Init

  RadioCheckRfFrequency (Thumb, 6 bytes, Stack size 0 bytes, radio.o(i.RadioCheckRfFrequency))
  [Address Reference Count : 1]

  - radio.o(.constdata)

  RadioGetStatus (Thumb, 36 bytes, Stack size 4 bytes, radio.o(i.RadioGetStatus))
  [Stack]

  - Max Depth = 4
  - Call Chain = RadioGetStatus
  [Calls]
  - >> SX126xGetOperatingMode
  [Address Reference Count : 1]
  - radio.o(.constdata)

  RadioGetWakeupTime (Thumb, 10 bytes, Stack size 4 bytes, radio.o(i.RadioGetWakeupTime))
  [Stack]

  - Max Depth = 4
  - Call Chain = RadioGetWakeupTime
  [Calls]
  - >> SX126xGetBoardTcxoWakeupTime
  [Address Reference Count : 1]
  - radio.o(.constdata)

  RadioInit (Thumb, 72 bytes, Stack size 8 bytes, radio.o(i.RadioInit))
  [Stack]

  - Max Depth = 248 + Unknown Stack Size
  - Call Chain = RadioInit ⇒ SX126xSetTxParams ⇒ SX126xSetPaConfig ⇒ SX126xWriteCommand ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xSetTxParams
  - >> SX126xSetStandby
  - >> SX126xSetRegulatorMode
  - >> SX126xSetDioIrqParams
  - >> SX126xSetBufferBaseAddress
  - >> SX126xInit
  - >> SX126xTimerInit
  - >> SX126xIoInit
  [Address Reference Count : 1]
  - radio.o(.constdata)

  RadioIrqProcess (Thumb, 410 bytes, Stack size 16 bytes, radio.o(i.RadioIrqProcess))
  [Stack]

  - Max Depth = 264 + Unknown Stack Size
  - Call Chain = RadioIrqProcess ⇒ SX126xGetPayload ⇒ SX126xGetRxBufferStatus ⇒ SX126xReadRegister ⇒ SX126xReadRegisters ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xGetPayload
  - >> SX126xGetPacketStatus
  - >> SX126xGetIrqStatus
  - >> SX126xClearIrqStatus
  - >> SX126xWriteRegister
  - >> SX126xSetOperatingMode
  - >> SX126xReadRegister
  - >> SX126xGetOperatingMode
  - >> SX126xTxTimerStop
  - >> SX126xRxTimerStop
  [Address Reference Count : 1]
  - radio.o(.constdata)

  RadioIsChannelFree (Thumb, 136 bytes, Stack size 72 bytes, radio.o(i.RadioIsChannelFree))
  [Stack]

  - Max Depth = 360 + Unknown Stack Size
  - Call Chain = RadioIsChannelFree ⇒ RadioSetRxConfig ⇒ SX126xSetPacketParams ⇒ SX126xSetCrcSeed ⇒ SX126xWriteRegisters ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> RadioSleep
  - >> RadioSetRxConfig
  - >> RadioSetModem
  - >> RadioSetChannel
  - >> RadioRx
  - >> RadioRssi
  - >> SX126xDelayMs
  [Address Reference Count : 1]
  - radio.o(.constdata)

  RadioOnDioIrq (Thumb, 8 bytes, Stack size 0 bytes, radio.o(i.RadioOnDioIrq))
  [Address Reference Count : 1]

  - radio.o(i.RadioInit)

  RadioOnRxTimeoutIrq (Thumb, 28 bytes, Stack size 8 bytes, radio.o(i.RadioOnRxTimeoutIrq))
  [Stack]

  - Max Depth = 8
  - Call Chain = RadioOnRxTimeoutIrq
  [Called By]
  - >> TIM3_IRQHandler

  RadioOnTxTimeoutIrq (Thumb, 28 bytes, Stack size 8 bytes, radio.o(i.RadioOnTxTimeoutIrq))
  [Stack]

  - Max Depth = 8
  - Call Chain = RadioOnTxTimeoutIrq
  [Called By]
  - >> TIM3_IRQHandler

  RadioRandom (Thumb, 32 bytes, Stack size 8 bytes, radio.o(i.RadioRandom))
  [Stack]

  - Max Depth = 232 + Unknown Stack Size
  - Call Chain = RadioRandom ⇒ SX126xSetDioIrqParams ⇒ SX126xWriteCommand ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xSetDioIrqParams
  - >> SX126xGetRandom
  - >> RadioSetModem
  [Address Reference Count : 1]
  - radio.o(.constdata)

  RadioRead (Thumb, 12 bytes, Stack size 8 bytes, radio.o(i.RadioRead))
  [Stack]

  - Max Depth = 216 + Unknown Stack Size
  - Call Chain = RadioRead ⇒ SX126xReadRegister ⇒ SX126xReadRegisters ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xReadRegister
  [Address Reference Count : 1]
  - radio.o(.constdata)

  RadioReadBuffer (Thumb, 20 bytes, Stack size 16 bytes, radio.o(i.RadioReadBuffer))
  [Stack]

  - Max Depth = 208 + Unknown Stack Size
  - Call Chain = RadioReadBuffer ⇒ SX126xReadRegisters ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xReadRegisters
  [Address Reference Count : 1]
  - radio.o(.constdata)

  RadioRssi (Thumb, 10 bytes, Stack size 8 bytes, radio.o(i.RadioRssi))
  [Stack]

  - Max Depth = 216 + Unknown Stack Size
  - Call Chain = RadioRssi ⇒ SX126xGetRssiInst ⇒ SX126xReadCommand ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xGetRssiInst
  [Called By]
  - >> RadioIsChannelFree
  [Address Reference Count : 1]
  - radio.o(.constdata)

  RadioRx (Thumb, 60 bytes, Stack size 8 bytes, radio.o(i.RadioRx))
  [Stack]

  - Max Depth = 232 + Unknown Stack Size
  - Call Chain = RadioRx ⇒ SX126xSetDioIrqParams ⇒ SX126xWriteCommand ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xSetRx
  - >> SX126xSetDioIrqParams
  - >> SX126xSetRxTimerValue
  - >> SX126xRxTimerStart
  [Called By]
  - >> RadioIsChannelFree
  [Address Reference Count : 1]
  - radio.o(.constdata)

  RadioRxBoosted (Thumb, 60 bytes, Stack size 8 bytes, radio.o(i.RadioRxBoosted))
  [Stack]

  - Max Depth = 232 + Unknown Stack Size
  - Call Chain = RadioRxBoosted ⇒ SX126xSetRxBoosted ⇒ SX126xWriteRegister ⇒ SX126xWriteRegisters ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xSetRxBoosted
  - >> SX126xSetDioIrqParams
  - >> SX126xSetRxTimerValue
  - >> SX126xRxTimerStart
  [Address Reference Count : 1]
  - radio.o(.constdata)

  RadioSend (Thumb, 68 bytes, Stack size 16 bytes, radio.o(i.RadioSend))
  [Stack]

  - Max Depth = 256 + Unknown Stack Size
  - Call Chain = RadioSend ⇒ SX126xSetPacketParams ⇒ SX126xSetCrcSeed ⇒ SX126xWriteRegisters ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xSetPacketParams
  - >> SX126xSetDioIrqParams
  - >> SX126xSendPayload
  - >> SX126xGetPacketType
  - >> SX126xTxTimerStart
  - >> SX126xSetTxTimerValue
  [Address Reference Count : 1]
  - radio.o(.constdata)

  RadioSetChannel (Thumb, 12 bytes, Stack size 8 bytes, radio.o(i.RadioSetChannel))
  [Stack]

  - Max Depth = 232 + Unknown Stack Size
  - Call Chain = RadioSetChannel ⇒ SX126xSetRfFrequency ⇒ SX126xCalibrateImage ⇒ SX126xWriteCommand ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xSetRfFrequency
  [Called By]
  - >> RadioIsChannelFree
  [Address Reference Count : 1]
  - radio.o(.constdata)

  RadioSetMaxPayloadLength (Thumb, 46 bytes, Stack size 16 bytes, radio.o(i.RadioSetMaxPayloadLength))
  [Stack]

  - Max Depth = 256 + Unknown Stack Size
  - Call Chain = RadioSetMaxPayloadLength ⇒ SX126xSetPacketParams ⇒ SX126xSetCrcSeed ⇒ SX126xWriteRegisters ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xSetPacketParams
  [Address Reference Count : 1]
  - radio.o(.constdata)

  RadioSetModem (Thumb, 64 bytes, Stack size 8 bytes, radio.o(i.RadioSetModem))
  [Stack]

  - Max Depth = 224 + Unknown Stack Size
  - Call Chain = RadioSetModem ⇒ RadioSetPublicNetwork ⇒ RadioSetModem (Cycle)
  [Calls]
  - >> SX126xSetPacketType
  - >> RadioSetPublicNetwork
  [Called By]
  - >> RadioSetTxConfig
  - >> RadioSetRxConfig
  - >> RadioSetPublicNetwork
  - >> RadioRandom
  - >> RadioIsChannelFree
  [Address Reference Count : 1]
  - radio.o(.constdata)

  RadioSetPublicNetwork (Thumb, 64 bytes, Stack size 8 bytes, radio.o(i.RadioSetPublicNetwork))
  [Stack]

  - Max Depth = 232 + Unknown Stack Size + In Cycle
  - Call Chain = RadioSetPublicNetwork ⇒ RadioSetModem (Cycle)
  [Calls]
  - >> SX126xWriteRegister
  - >> RadioSetModem
  [Called By]
  - >> RadioSetModem
  [Address Reference Count : 1]
  - radio.o(.constdata)

  RadioSetRxConfig (Thumb, 512 bytes, Stack size 48 bytes, radio.o(i.RadioSetRxConfig))
  [Stack]

  - Max Depth = 288 + Unknown Stack Size
  - Call Chain = RadioSetRxConfig ⇒ SX126xSetPacketParams ⇒ SX126xSetCrcSeed ⇒ SX126xWriteRegisters ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xSetWhiteningSeed
  - >> SX126xSetSyncWord
  - >> SX126xSetStopRxTimerOnPreambleDetect
  - >> SX126xSetPacketParams
  - >> SX126xSetModulationParams
  - >> SX126xSetLoRaSymbNumTimeout
  - >> SX126xWriteRegister
  - >> SX126xReadRegister
  - >> RadioStandby
  - >> RadioSetModem
  - >> RadioGetFskBandwidthRegValue
  [Called By]
  - >> RadioIsChannelFree
  [Address Reference Count : 1]
  - radio.o(.constdata)

  RadioSetRxDutyCycle (Thumb, 16 bytes, Stack size 16 bytes, radio.o(i.RadioSetRxDutyCycle))
  [Stack]

  - Max Depth = 232 + Unknown Stack Size
  - Call Chain = RadioSetRxDutyCycle ⇒ SX126xSetRxDutyCycle ⇒ SX126xWriteCommand ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xSetRxDutyCycle
  [Address Reference Count : 1]
  - radio.o(.constdata)

  RadioSetTxConfig (Thumb, 444 bytes, Stack size 48 bytes, radio.o(i.RadioSetTxConfig))
  [Stack]

  - Max Depth = 296 + Unknown Stack Size
  - Call Chain = RadioSetTxConfig ⇒ SX126xSetRfTxPower ⇒ SX126xSetTxParams ⇒ SX126xSetPaConfig ⇒ SX126xWriteCommand ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xSetWhiteningSeed
  - >> SX126xSetSyncWord
  - >> SX126xSetPacketParams
  - >> SX126xSetModulationParams
  - >> SX126xWriteRegister
  - >> SX126xSetRfTxPower
  - >> SX126xReadRegister
  - >> RadioStandby
  - >> RadioSetModem
  - >> RadioGetFskBandwidthRegValue
  [Address Reference Count : 1]
  - radio.o(.constdata)

  RadioSetTxContinuousWave (Thumb, 48 bytes, Stack size 24 bytes, radio.o(i.RadioSetTxContinuousWave))
  [Stack]

  - Max Depth = 272 + Unknown Stack Size
  - Call Chain = RadioSetTxContinuousWave ⇒ SX126xSetRfTxPower ⇒ SX126xSetTxParams ⇒ SX126xSetPaConfig ⇒ SX126xWriteCommand ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xSetTxContinuousWave
  - >> SX126xSetRfFrequency
  - >> SX126xSetRfTxPower
  - >> SX126xTxTimerStart
  - >> SX126xSetTxTimerValue
  [Address Reference Count : 1]
  - radio.o(.constdata)

  RadioSleep (Thumb, 32 bytes, Stack size 8 bytes, radio.o(i.RadioSleep))
  [Stack]

  - Max Depth = 216 + Unknown Stack Size
  - Call Chain = RadioSleep ⇒ SX126xSetSleep ⇒ SX126xWriteCommand ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xSetSleep
  - >> SX126xDelayMs
  [Called By]
  - >> RadioIsChannelFree
  [Address Reference Count : 1]
  - radio.o(.constdata)

  RadioStandby (Thumb, 10 bytes, Stack size 8 bytes, radio.o(i.RadioStandby))
  [Stack]

  - Max Depth = 208 + Unknown Stack Size
  - Call Chain = RadioStandby ⇒ SX126xSetStandby ⇒ SX126xWriteCommand ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xSetStandby
  [Called By]
  - >> RadioSetTxConfig
  - >> RadioSetRxConfig
  [Address Reference Count : 1]
  - radio.o(.constdata)

  RadioStartCad (Thumb, 22 bytes, Stack size 8 bytes, radio.o(i.RadioStartCad))
  [Stack]

  - Max Depth = 232 + Unknown Stack Size
  - Call Chain = RadioStartCad ⇒ SX126xSetDioIrqParams ⇒ SX126xWriteCommand ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xSetDioIrqParams
  - >> SX126xSetCad
  [Address Reference Count : 1]
  - radio.o(.constdata)

  RadioTimeOnAir (Thumb, 118 bytes, Stack size 48 bytes, radio.o(i.RadioTimeOnAir))
  [Stack]

  - Max Depth = 84
  - Call Chain = RadioTimeOnAir ⇒ RadioGetLoRaTimeOnAirNumerator
  [Calls]
  - >> RadioGetLoRaTimeOnAirNumerator
  - >> RadioGetLoRaBandwidthInHz
  - >> RadioGetGfskTimeOnAirNumerator
  [Address Reference Count : 1]
  - radio.o(.constdata)

  RadioWrite (Thumb, 16 bytes, Stack size 16 bytes, radio.o(i.RadioWrite))
  [Stack]

  - Max Depth = 224 + Unknown Stack Size
  - Call Chain = RadioWrite ⇒ SX126xWriteRegister ⇒ SX126xWriteRegisters ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xWriteRegister
  [Address Reference Count : 1]
  - radio.o(.constdata)

  RadioWriteBuffer (Thumb, 20 bytes, Stack size 16 bytes, radio.o(i.RadioWriteBuffer))
  [Stack]

  - Max Depth = 208 + Unknown Stack Size
  - Call Chain = RadioWriteBuffer ⇒ SX126xWriteRegisters ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xWriteRegisters
  [Address Reference Count : 1]
  - radio.o(.constdata)

  SPI_Cmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_spi.o(i.SPI_Cmd))
  [Called By]

  - >> Spi1Init

  SPI_I2S_GetFlagStatus (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_spi.o(i.SPI_I2S_GetFlagStatus))
  [Called By]

  - >> HALSpi1InOut

  SPI_I2S_ReceiveData (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_spi.o(i.SPI_I2S_ReceiveData))
  [Called By]

  - >> HALSpi1InOut

  SPI_I2S_SendData (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_spi.o(i.SPI_I2S_SendData))
  [Called By]

  - >> HALSpi1InOut

  SPI_Init (Thumb, 60 bytes, Stack size 8 bytes, stm32f10x_spi.o(i.SPI_Init))
  [Stack]

  - Max Depth = 8
  - Call Chain = SPI_Init
  [Called By]
  - >> Spi1Init

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.SVC_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SX126xAntSwOff (Thumb, 2 bytes, Stack size 0 bytes, radio.o(i.SX126xAntSwOff))
  [Called By]

  - >> SX126xSetSleep

  SX126xAntSwOn (Thumb, 2 bytes, Stack size 0 bytes, radio.o(i.SX126xAntSwOn))
  [Called By]

  - >> SX126xCheckDeviceReady

  SX126xCalibrateImage (Thumb, 114 bytes, Stack size 16 bytes, sx126x.o(i.SX126xCalibrateImage))
  [Stack]

  - Max Depth = 208 + Unknown Stack Size
  - Call Chain = SX126xCalibrateImage ⇒ SX126xWriteCommand ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xWriteCommand
  [Called By]
  - >> SX126xSetRfFrequency

  SX126xCheckDeviceReady (Thumb, 30 bytes, Stack size 8 bytes, sx126x.o(i.SX126xCheckDeviceReady))
  [Stack]

  - Max Depth = 168 + Unknown Stack Size
  - Call Chain = SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xWakeup
  - >> SX126xGetOperatingMode
  - >> SX126xAntSwOn
  - >> SX126xWaitOnBusy
  [Called By]
  - >> SX126xWriteRegisters
  - >> SX126xWriteCommand
  - >> SX126xWriteBuffer
  - >> SX126xReadRegisters
  - >> SX126xReadCommand
  - >> SX126xReadBuffer

  SX126xClearIrqStatus (Thumb, 28 bytes, Stack size 16 bytes, sx126x.o(i.SX126xClearIrqStatus))
  [Stack]

  - Max Depth = 208 + Unknown Stack Size
  - Call Chain = SX126xClearIrqStatus ⇒ SX126xWriteCommand ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xWriteCommand
  [Called By]
  - >> RadioIrqProcess

  SX126xDelayMs (Thumb, 12 bytes, Stack size 8 bytes, sx126xstm32f103-board.o(i.SX126xDelayMs))
  [Stack]

  - Max Depth = 16
  - Call Chain = SX126xDelayMs ⇒ delay_ms
  [Calls]
  - >> delay_ms
  [Called By]
  - >> RadioSleep
  - >> RadioIsChannelFree
  - >> SX126xWaitOnBusy
  - >> SX126xReset

  SX126xGetBoardTcxoWakeupTime (Thumb, 4 bytes, Stack size 0 bytes, radio.o(i.SX126xGetBoardTcxoWakeupTime))
  [Called By]

  - >> RadioGetWakeupTime

  SX126xGetDeviceId (Thumb, 4 bytes, Stack size 0 bytes, radio.o(i.SX126xGetDeviceId))
  [Called By]

  - >> SX126xSetTxParams

  SX126xGetIrqStatus (Thumb, 26 bytes, Stack size 8 bytes, sx126x.o(i.SX126xGetIrqStatus))
  [Stack]

  - Max Depth = 200 + Unknown Stack Size
  - Call Chain = SX126xGetIrqStatus ⇒ SX126xReadCommand ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xReadCommand
  [Called By]
  - >> RadioIrqProcess

  SX126xGetOperatingMode (Thumb, 6 bytes, Stack size 0 bytes, radio.o(i.SX126xGetOperatingMode))
  [Called By]

  - >> SX126xCheckDeviceReady
  - >> RadioIrqProcess
  - >> RadioGetStatus

  SX126xGetPacketStatus (Thumb, 134 bytes, Stack size 16 bytes, sx126x.o(i.SX126xGetPacketStatus))
  [Stack]

  - Max Depth = 208 + Unknown Stack Size
  - Call Chain = SX126xGetPacketStatus ⇒ SX126xReadCommand ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xGetPacketType
  - >> SX126xReadCommand
  - >> __aeabi_memclr4
  [Called By]
  - >> RadioIrqProcess

  SX126xGetPacketType (Thumb, 6 bytes, Stack size 0 bytes, sx126x.o(i.SX126xGetPacketType))
  [Called By]

  - >> SX126xSetWhiteningSeed
  - >> SX126xGetPacketStatus
  - >> RadioSend
  - >> SX126xSetCrcSeed
  - >> SX126xSetCrcPolynomial
  - >> SX126xGetRxBufferStatus

  SX126xGetPayload (Thumb, 46 bytes, Stack size 24 bytes, sx126x.o(i.SX126xGetPayload))
  [Stack]

  - Max Depth = 248 + Unknown Stack Size
  - Call Chain = SX126xGetPayload ⇒ SX126xGetRxBufferStatus ⇒ SX126xReadRegister ⇒ SX126xReadRegisters ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xReadBuffer
  - >> SX126xGetRxBufferStatus
  [Called By]
  - >> RadioIrqProcess

  SX126xGetRandom (Thumb, 104 bytes, Stack size 16 bytes, sx126x.o(i.SX126xGetRandom))
  [Stack]

  - Max Depth = 224 + Unknown Stack Size
  - Call Chain = SX126xGetRandom ⇒ SX126xSetRx ⇒ SX126xWriteCommand ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xSetStandby
  - >> SX126xSetRx
  - >> SX126xWriteRegister
  - >> SX126xReadRegisters
  - >> SX126xReadRegister
  [Called By]
  - >> RadioRandom

  SX126xGetRssiInst (Thumb, 28 bytes, Stack size 16 bytes, sx126x.o(i.SX126xGetRssiInst))
  [Stack]

  - Max Depth = 208 + Unknown Stack Size
  - Call Chain = SX126xGetRssiInst ⇒ SX126xReadCommand ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xReadCommand
  [Called By]
  - >> RadioRssi

  SX126xGetRxBufferStatus (Thumb, 58 bytes, Stack size 16 bytes, sx126x.o(i.SX126xGetRxBufferStatus))
  [Stack]

  - Max Depth = 224 + Unknown Stack Size
  - Call Chain = SX126xGetRxBufferStatus ⇒ SX126xReadRegister ⇒ SX126xReadRegisters ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xGetPacketType
  - >> SX126xReadRegister
  - >> SX126xReadCommand
  [Called By]
  - >> SX126xGetPayload

  SX126xInit (Thumb, 40 bytes, Stack size 8 bytes, sx126x.o(i.SX126xInit))
  [Stack]

  - Max Depth = 216 + Unknown Stack Size
  - Call Chain = SX126xInit ⇒ SX126xIoRfSwitchInit ⇒ SX126xSetDio2AsRfSwitchCtrl ⇒ SX126xWriteCommand ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xSetStandby
  - >> SX126xWakeup
  - >> SX126xSetOperatingMode
  - >> SX126xIoTcxoInit
  - >> SX126xIoRfSwitchInit
  - >> SX126xReset
  - >> SX126xIoIrqInit
  [Called By]
  - >> RadioInit

  SX126xIoInit (Thumb, 126 bytes, Stack size 16 bytes, sx126xstm32f103-board.o(i.SX126xIoInit))
  [Stack]

  - Max Depth = 160 + Unknown Stack Size
  - Call Chain = SX126xIoInit ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_Init
  - >> Spi1Init
  - >> __2printf
  [Called By]
  - >> RadioInit

  SX126xIoIrqInit (Thumb, 130 bytes, Stack size 24 bytes, sx126xstm32f103-board.o(i.SX126xIoIrqInit))
  [Stack]

  - Max Depth = 48
  - Call Chain = SX126xIoIrqInit ⇒ GPIO_Init
  [Calls]
  - >> GPIO_EXTILineConfig
  - >> NVIC_Init
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_Init
  - >> EXTI_Init
  - >> EXTI_ClearITPendingBit
  [Called By]
  - >> SX126xInit

  SX126xIoRfSwitchInit (Thumb, 10 bytes, Stack size 8 bytes, radio.o(i.SX126xIoRfSwitchInit))
  [Stack]

  - Max Depth = 208 + Unknown Stack Size
  - Call Chain = SX126xIoRfSwitchInit ⇒ SX126xSetDio2AsRfSwitchCtrl ⇒ SX126xWriteCommand ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xSetDio2AsRfSwitchCtrl
  [Called By]
  - >> SX126xInit

  SX126xIoTcxoInit (Thumb, 2 bytes, Stack size 0 bytes, radio.o(i.SX126xIoTcxoInit))
  [Called By]

  - >> SX126xInit

  SX126xReadBuffer (Thumb, 74 bytes, Stack size 24 bytes, radio.o(i.SX126xReadBuffer))
  [Stack]

  - Max Depth = 192 + Unknown Stack Size
  - Call Chain = SX126xReadBuffer ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xCheckDeviceReady
  - >> SX126xWaitOnBusy
  - >> SX126xSpiInOut
  - >> SX126xSetNss
  [Called By]
  - >> SX126xGetPayload

  SX126xReadCommand (Thumb, 76 bytes, Stack size 24 bytes, radio.o(i.SX126xReadCommand))
  [Stack]

  - Max Depth = 192 + Unknown Stack Size
  - Call Chain = SX126xReadCommand ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xCheckDeviceReady
  - >> SX126xWaitOnBusy
  - >> SX126xSpiInOut
  - >> SX126xSetNss
  [Called By]
  - >> SX126xGetRssiInst
  - >> SX126xGetPacketStatus
  - >> SX126xGetIrqStatus
  - >> SX126xGetRxBufferStatus

  SX126xReadRegister (Thumb, 20 bytes, Stack size 16 bytes, radio.o(i.SX126xReadRegister))
  [Stack]

  - Max Depth = 208 + Unknown Stack Size
  - Call Chain = SX126xReadRegister ⇒ SX126xReadRegisters ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xReadRegisters
  [Called By]
  - >> SX126xSetWhiteningSeed
  - >> SX126xSetTxParams
  - >> SX126xGetRandom
  - >> RadioSetTxConfig
  - >> RadioSetRxConfig
  - >> RadioRead
  - >> RadioIrqProcess
  - >> SX126xGetRxBufferStatus

  SX126xReadRegisters (Thumb, 80 bytes, Stack size 24 bytes, radio.o(i.SX126xReadRegisters))
  [Stack]

  - Max Depth = 192 + Unknown Stack Size
  - Call Chain = SX126xReadRegisters ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xCheckDeviceReady
  - >> SX126xWaitOnBusy
  - >> SX126xSpiInOut
  - >> SX126xSetNss
  [Called By]
  - >> SX126xGetRandom
  - >> SX126xReadRegister
  - >> RadioReadBuffer

  SX126xReset (Thumb, 80 bytes, Stack size 8 bytes, sx126xstm32f103-board.o(i.SX126xReset))
  [Stack]

  - Max Depth = 32
  - Call Chain = SX126xReset ⇒ GPIO_Init
  [Calls]
  - >> GPIO_WriteBit
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_Init
  - >> SX126xDelayMs
  [Called By]
  - >> SX126xInit

  SX126xRxTimerStart (Thumb, 28 bytes, Stack size 8 bytes, sx126xstm32f103-board.o(i.SX126xRxTimerStart))
  [Stack]

  - Max Depth = 152 + Unknown Stack Size
  - Call Chain = SX126xRxTimerStart ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> __2printf
  [Called By]
  - >> RadioRxBoosted
  - >> RadioRx

  SX126xRxTimerStop (Thumb, 22 bytes, Stack size 8 bytes, sx126xstm32f103-board.o(i.SX126xRxTimerStop))
  [Stack]

  - Max Depth = 152 + Unknown Stack Size
  - Call Chain = SX126xRxTimerStop ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> __2printf
  [Called By]
  - >> RadioIrqProcess
  - >> TIM3_IRQHandler

  SX126xSendPayload (Thumb, 24 bytes, Stack size 16 bytes, sx126x.o(i.SX126xSendPayload))
  [Stack]

  - Max Depth = 224 + Unknown Stack Size
  - Call Chain = SX126xSendPayload ⇒ SX126xSetTx ⇒ SX126xWriteCommand ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xSetTx
  - >> SX126xSetPayload
  [Called By]
  - >> RadioSend

  SX126xSetBufferBaseAddress (Thumb, 26 bytes, Stack size 16 bytes, sx126x.o(i.SX126xSetBufferBaseAddress))
  [Stack]

  - Max Depth = 208 + Unknown Stack Size
  - Call Chain = SX126xSetBufferBaseAddress ⇒ SX126xWriteCommand ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xWriteCommand
  [Called By]
  - >> RadioInit

  SX126xSetCad (Thumb, 20 bytes, Stack size 8 bytes, sx126x.o(i.SX126xSetCad))
  [Stack]

  - Max Depth = 200 + Unknown Stack Size
  - Call Chain = SX126xSetCad ⇒ SX126xWriteCommand ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xWriteCommand
  - >> SX126xSetOperatingMode
  [Called By]
  - >> RadioStartCad

  SX126xSetCrcPolynomial (Thumb, 42 bytes, Stack size 16 bytes, sx126x.o(i.SX126xSetCrcPolynomial))
  [Stack]

  - Max Depth = 208 + Unknown Stack Size
  - Call Chain = SX126xSetCrcPolynomial ⇒ SX126xWriteRegisters ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xGetPacketType
  - >> SX126xWriteRegisters
  [Called By]
  - >> SX126xSetPacketParams

  SX126xSetCrcSeed (Thumb, 42 bytes, Stack size 16 bytes, sx126x.o(i.SX126xSetCrcSeed))
  [Stack]

  - Max Depth = 208 + Unknown Stack Size
  - Call Chain = SX126xSetCrcSeed ⇒ SX126xWriteRegisters ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xGetPacketType
  - >> SX126xWriteRegisters
  [Called By]
  - >> SX126xSetPacketParams

  SX126xSetDio2AsRfSwitchCtrl (Thumb, 14 bytes, Stack size 8 bytes, sx126x.o(i.SX126xSetDio2AsRfSwitchCtrl))
  [Stack]

  - Max Depth = 200 + Unknown Stack Size
  - Call Chain = SX126xSetDio2AsRfSwitchCtrl ⇒ SX126xWriteCommand ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xWriteCommand
  [Called By]
  - >> SX126xIoRfSwitchInit

  SX126xSetDioIrqParams (Thumb, 74 bytes, Stack size 32 bytes, sx126x.o(i.SX126xSetDioIrqParams))
  [Stack]

  - Max Depth = 224 + Unknown Stack Size
  - Call Chain = SX126xSetDioIrqParams ⇒ SX126xWriteCommand ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xWriteCommand
  [Called By]
  - >> RadioStartCad
  - >> RadioSend
  - >> RadioRxBoosted
  - >> RadioRx
  - >> RadioRandom
  - >> RadioInit

  SX126xSetLoRaSymbNumTimeout (Thumb, 84 bytes, Stack size 24 bytes, sx126x.o(i.SX126xSetLoRaSymbNumTimeout))
  [Stack]

  - Max Depth = 232 + Unknown Stack Size
  - Call Chain = SX126xSetLoRaSymbNumTimeout ⇒ SX126xWriteRegister ⇒ SX126xWriteRegisters ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xWriteRegister
  - >> SX126xWriteCommand
  [Called By]
  - >> RadioSetRxConfig

  SX126xSetModulationParams (Thumb, 168 bytes, Stack size 24 bytes, sx126x.o(i.SX126xSetModulationParams))
  [Stack]

  - Max Depth = 224 + Unknown Stack Size
  - Call Chain = SX126xSetModulationParams ⇒ SX126xSetPacketType ⇒ SX126xWriteCommand ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xSetPacketType
  - >> SX126xWriteCommand
  - >> SX126xConvertFreqInHzToPllStep
  [Called By]
  - >> RadioSetTxConfig
  - >> RadioSetRxConfig

  SX126xSetNss (Thumb, 26 bytes, Stack size 8 bytes, sx126xstm32f103-board.o(i.SX126xSetNss))
  [Stack]

  - Max Depth = 8
  - Call Chain = SX126xSetNss
  [Calls]
  - >> GPIO_SetBits
  - >> GPIO_ResetBits
  [Called By]
  - >> SX126xWriteRegisters
  - >> SX126xWriteCommand
  - >> SX126xWriteBuffer
  - >> SX126xWakeup
  - >> SX126xReadRegisters
  - >> SX126xReadCommand
  - >> SX126xReadBuffer

  SX126xSetOperatingMode (Thumb, 6 bytes, Stack size 0 bytes, radio.o(i.SX126xSetOperatingMode))
  [Called By]

  - >> SX126xSetTxContinuousWave
  - >> SX126xSetStandby
  - >> SX126xSetSleep
  - >> SX126xSetRxDutyCycle
  - >> SX126xSetRxBoosted
  - >> SX126xSetRx
  - >> SX126xSetCad
  - >> SX126xInit
  - >> SX126xWakeup
  - >> RadioIrqProcess
  - >> SX126xSetTx

  SX126xSetPaConfig (Thumb, 38 bytes, Stack size 24 bytes, sx126x.o(i.SX126xSetPaConfig))
  [Stack]

  - Max Depth = 216 + Unknown Stack Size
  - Call Chain = SX126xSetPaConfig ⇒ SX126xWriteCommand ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xWriteCommand
  [Called By]
  - >> SX126xSetTxParams

  SX126xSetPacketParams (Thumb, 222 bytes, Stack size 32 bytes, sx126x.o(i.SX126xSetPacketParams))
  [Stack]

  - Max Depth = 240 + Unknown Stack Size
  - Call Chain = SX126xSetPacketParams ⇒ SX126xSetCrcSeed ⇒ SX126xWriteRegisters ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xSetPacketType
  - >> SX126xWriteCommand
  - >> SX126xSetCrcSeed
  - >> SX126xSetCrcPolynomial
  [Called By]
  - >> RadioSetTxConfig
  - >> RadioSetRxConfig
  - >> RadioSetMaxPayloadLength
  - >> RadioSend

  SX126xSetPacketType (Thumb, 22 bytes, Stack size 8 bytes, sx126x.o(i.SX126xSetPacketType))
  [Stack]

  - Max Depth = 200 + Unknown Stack Size
  - Call Chain = SX126xSetPacketType ⇒ SX126xWriteCommand ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xWriteCommand
  [Called By]
  - >> SX126xSetPacketParams
  - >> SX126xSetModulationParams
  - >> RadioSetModem

  SX126xSetPayload (Thumb, 18 bytes, Stack size 16 bytes, sx126x.o(i.SX126xSetPayload))
  [Stack]

  - Max Depth = 208 + Unknown Stack Size
  - Call Chain = SX126xSetPayload ⇒ SX126xWriteBuffer ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xWriteBuffer
  [Called By]
  - >> SX126xSendPayload

  SX126xSetRegulatorMode (Thumb, 14 bytes, Stack size 8 bytes, sx126x.o(i.SX126xSetRegulatorMode))
  [Stack]

  - Max Depth = 200 + Unknown Stack Size
  - Call Chain = SX126xSetRegulatorMode ⇒ SX126xWriteCommand ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xWriteCommand
  [Called By]
  - >> RadioInit

  SX126xSetRfFrequency (Thumb, 68 bytes, Stack size 16 bytes, sx126x.o(i.SX126xSetRfFrequency))
  [Stack]

  - Max Depth = 224 + Unknown Stack Size
  - Call Chain = SX126xSetRfFrequency ⇒ SX126xCalibrateImage ⇒ SX126xWriteCommand ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xWriteCommand
  - >> SX126xCalibrateImage
  - >> SX126xConvertFreqInHzToPllStep
  [Called By]
  - >> RadioSetTxContinuousWave
  - >> RadioSetChannel

  SX126xSetRfTxPower (Thumb, 14 bytes, Stack size 8 bytes, radio.o(i.SX126xSetRfTxPower))
  [Stack]

  - Max Depth = 248 + Unknown Stack Size
  - Call Chain = SX126xSetRfTxPower ⇒ SX126xSetTxParams ⇒ SX126xSetPaConfig ⇒ SX126xWriteCommand ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xSetTxParams
  [Called By]
  - >> RadioSetTxContinuousWave
  - >> RadioSetTxConfig

  SX126xSetRx (Thumb, 40 bytes, Stack size 16 bytes, sx126x.o(i.SX126xSetRx))
  [Stack]

  - Max Depth = 208 + Unknown Stack Size
  - Call Chain = SX126xSetRx ⇒ SX126xWriteCommand ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xWriteCommand
  - >> SX126xSetOperatingMode
  [Called By]
  - >> SX126xGetRandom
  - >> RadioRx

  SX126xSetRxBoosted (Thumb, 50 bytes, Stack size 16 bytes, sx126x.o(i.SX126xSetRxBoosted))
  [Stack]

  - Max Depth = 224 + Unknown Stack Size
  - Call Chain = SX126xSetRxBoosted ⇒ SX126xWriteRegister ⇒ SX126xWriteRegisters ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xWriteRegister
  - >> SX126xWriteCommand
  - >> SX126xSetOperatingMode
  [Called By]
  - >> RadioRxBoosted

  SX126xSetRxDutyCycle (Thumb, 60 bytes, Stack size 24 bytes, sx126x.o(i.SX126xSetRxDutyCycle))
  [Stack]

  - Max Depth = 216 + Unknown Stack Size
  - Call Chain = SX126xSetRxDutyCycle ⇒ SX126xWriteCommand ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xWriteCommand
  - >> SX126xSetOperatingMode
  [Called By]
  - >> RadioSetRxDutyCycle

  SX126xSetRxTimerValue (Thumb, 24 bytes, Stack size 8 bytes, sx126xstm32f103-board.o(i.SX126xSetRxTimerValue))
  [Stack]

  - Max Depth = 152 + Unknown Stack Size
  - Call Chain = SX126xSetRxTimerValue ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> __2printf
  [Called By]
  - >> RadioRxBoosted
  - >> RadioRx

  SX126xSetSleep (Thumb, 64 bytes, Stack size 16 bytes, sx126x.o(i.SX126xSetSleep))
  [Stack]

  - Max Depth = 208 + Unknown Stack Size
  - Call Chain = SX126xSetSleep ⇒ SX126xWriteCommand ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xWriteCommand
  - >> SX126xSetOperatingMode
  - >> SX126xAntSwOff
  [Called By]
  - >> RadioSleep

  SX126xSetStandby (Thumb, 34 bytes, Stack size 8 bytes, sx126x.o(i.SX126xSetStandby))
  [Stack]

  - Max Depth = 200 + Unknown Stack Size
  - Call Chain = SX126xSetStandby ⇒ SX126xWriteCommand ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xWriteCommand
  - >> SX126xSetOperatingMode
  [Called By]
  - >> SX126xInit
  - >> SX126xGetRandom
  - >> RadioStandby
  - >> RadioInit

  SX126xSetStopRxTimerOnPreambleDetect (Thumb, 14 bytes, Stack size 8 bytes, sx126x.o(i.SX126xSetStopRxTimerOnPreambleDetect))
  [Stack]

  - Max Depth = 200 + Unknown Stack Size
  - Call Chain = SX126xSetStopRxTimerOnPreambleDetect ⇒ SX126xWriteCommand ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xWriteCommand
  [Called By]
  - >> RadioSetRxConfig

  SX126xSetSyncWord (Thumb, 20 bytes, Stack size 8 bytes, sx126x.o(i.SX126xSetSyncWord))
  [Stack]

  - Max Depth = 200 + Unknown Stack Size
  - Call Chain = SX126xSetSyncWord ⇒ SX126xWriteRegisters ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xWriteRegisters
  [Called By]
  - >> RadioSetTxConfig
  - >> RadioSetRxConfig

  SX126xSetTx (Thumb, 40 bytes, Stack size 16 bytes, sx126x.o(i.SX126xSetTx))
  [Stack]

  - Max Depth = 208 + Unknown Stack Size
  - Call Chain = SX126xSetTx ⇒ SX126xWriteCommand ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xWriteCommand
  - >> SX126xSetOperatingMode
  [Called By]
  - >> SX126xSendPayload

  SX126xSetTxContinuousWave (Thumb, 20 bytes, Stack size 8 bytes, sx126x.o(i.SX126xSetTxContinuousWave))
  [Stack]

  - Max Depth = 200 + Unknown Stack Size
  - Call Chain = SX126xSetTxContinuousWave ⇒ SX126xWriteCommand ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xWriteCommand
  - >> SX126xSetOperatingMode
  [Called By]
  - >> RadioSetTxContinuousWave

  SX126xSetTxParams (Thumb, 138 bytes, Stack size 24 bytes, sx126x.o(i.SX126xSetTxParams))
  [Stack]

  - Max Depth = 240 + Unknown Stack Size
  - Call Chain = SX126xSetTxParams ⇒ SX126xSetPaConfig ⇒ SX126xWriteCommand ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xWriteRegister
  - >> SX126xWriteCommand
  - >> SX126xReadRegister
  - >> SX126xGetDeviceId
  - >> SX126xSetPaConfig
  [Called By]
  - >> SX126xSetRfTxPower
  - >> RadioInit

  SX126xSetTxTimerValue (Thumb, 24 bytes, Stack size 8 bytes, sx126xstm32f103-board.o(i.SX126xSetTxTimerValue))
  [Stack]

  - Max Depth = 152 + Unknown Stack Size
  - Call Chain = SX126xSetTxTimerValue ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> __2printf
  [Called By]
  - >> RadioSetTxContinuousWave
  - >> RadioSend

  SX126xSetWhiteningSeed (Thumb, 58 bytes, Stack size 16 bytes, sx126x.o(i.SX126xSetWhiteningSeed))
  [Stack]

  - Max Depth = 224 + Unknown Stack Size
  - Call Chain = SX126xSetWhiteningSeed ⇒ SX126xWriteRegister ⇒ SX126xWriteRegisters ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xGetPacketType
  - >> SX126xWriteRegister
  - >> SX126xReadRegister
  [Called By]
  - >> RadioSetTxConfig
  - >> RadioSetRxConfig

  SX126xSpiInOut (Thumb, 12 bytes, Stack size 8 bytes, sx126xstm32f103-board.o(i.SX126xSpiInOut))
  [Stack]

  - Max Depth = 24
  - Call Chain = SX126xSpiInOut ⇒ HALSpi1InOut
  [Calls]
  - >> HALSpi1InOut
  [Called By]
  - >> SX126xWriteRegisters
  - >> SX126xWriteCommand
  - >> SX126xWriteBuffer
  - >> SX126xWakeup
  - >> SX126xReadRegisters
  - >> SX126xReadCommand
  - >> SX126xReadBuffer

  SX126xTimerInit (Thumb, 120 bytes, Stack size 24 bytes, sx126xstm32f103-board.o(i.SX126xTimerInit))
  [Stack]

  - Max Depth = 40
  - Call Chain = SX126xTimerInit ⇒ NVIC_Init
  [Calls]
  - >> NVIC_Init
  - >> RCC_APB1PeriphClockCmd
  - >> TIM_TimeBaseInit
  - >> TIM_ITConfig
  - >> TIM_Cmd
  - >> TIM_ClearITPendingBit
  [Called By]
  - >> RadioInit

  SX126xTxTimerStart (Thumb, 28 bytes, Stack size 8 bytes, sx126xstm32f103-board.o(i.SX126xTxTimerStart))
  [Stack]

  - Max Depth = 152 + Unknown Stack Size
  - Call Chain = SX126xTxTimerStart ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> __2printf
  [Called By]
  - >> RadioSetTxContinuousWave
  - >> RadioSend

  SX126xTxTimerStop (Thumb, 22 bytes, Stack size 8 bytes, sx126xstm32f103-board.o(i.SX126xTxTimerStop))
  [Stack]

  - Max Depth = 152 + Unknown Stack Size
  - Call Chain = SX126xTxTimerStop ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> __2printf
  [Called By]
  - >> RadioIrqProcess
  - >> TIM3_IRQHandler

  SX126xWaitOnBusy (Thumb, 44 bytes, Stack size 8 bytes, sx126xstm32f103-board.o(i.SX126xWaitOnBusy))
  [Stack]

  - Max Depth = 152 + Unknown Stack Size
  - Call Chain = SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> GPIO_ReadInputDataBit
  - >> SX126xDelayMs
  - >> __2printf
  [Called By]
  - >> SX126xCheckDeviceReady
  - >> SX126xWriteRegisters
  - >> SX126xWriteCommand
  - >> SX126xWriteBuffer
  - >> SX126xWakeup
  - >> SX126xReadRegisters
  - >> SX126xReadCommand
  - >> SX126xReadBuffer

  SX126xWakeup (Thumb, 38 bytes, Stack size 8 bytes, radio.o(i.SX126xWakeup))
  [Stack]

  - Max Depth = 160 + Unknown Stack Size
  - Call Chain = SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xSetOperatingMode
  - >> SX126xWaitOnBusy
  - >> SX126xSpiInOut
  - >> SX126xSetNss
  [Called By]
  - >> SX126xInit
  - >> SX126xCheckDeviceReady

  SX126xWriteBuffer (Thumb, 66 bytes, Stack size 24 bytes, radio.o(i.SX126xWriteBuffer))
  [Stack]

  - Max Depth = 192 + Unknown Stack Size
  - Call Chain = SX126xWriteBuffer ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xCheckDeviceReady
  - >> SX126xWaitOnBusy
  - >> SX126xSpiInOut
  - >> SX126xSetNss
  [Called By]
  - >> SX126xSetPayload

  SX126xWriteCommand (Thumb, 64 bytes, Stack size 24 bytes, radio.o(i.SX126xWriteCommand))
  [Stack]

  - Max Depth = 192 + Unknown Stack Size
  - Call Chain = SX126xWriteCommand ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xCheckDeviceReady
  - >> SX126xWaitOnBusy
  - >> SX126xSpiInOut
  - >> SX126xSetNss
  [Called By]
  - >> SX126xSetTxParams
  - >> SX126xSetTxContinuousWave
  - >> SX126xSetStopRxTimerOnPreambleDetect
  - >> SX126xSetStandby
  - >> SX126xSetSleep
  - >> SX126xSetRxDutyCycle
  - >> SX126xSetRxBoosted
  - >> SX126xSetRx
  - >> SX126xSetRfFrequency
  - >> SX126xSetRegulatorMode
  - >> SX126xSetPacketType
  - >> SX126xSetPacketParams
  - >> SX126xSetModulationParams
  - >> SX126xSetLoRaSymbNumTimeout
  - >> SX126xSetDioIrqParams
  - >> SX126xSetDio2AsRfSwitchCtrl
  - >> SX126xSetCad
  - >> SX126xSetBufferBaseAddress
  - >> SX126xClearIrqStatus
  - >> SX126xSetTx
  - >> SX126xSetPaConfig
  - >> SX126xCalibrateImage

  SX126xWriteRegister (Thumb, 16 bytes, Stack size 16 bytes, radio.o(i.SX126xWriteRegister))
  [Stack]

  - Max Depth = 208 + Unknown Stack Size
  - Call Chain = SX126xWriteRegister ⇒ SX126xWriteRegisters ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xWriteRegisters
  [Called By]
  - >> SX126xSetWhiteningSeed
  - >> SX126xSetTxParams
  - >> SX126xSetRxBoosted
  - >> SX126xSetLoRaSymbNumTimeout
  - >> SX126xGetRandom
  - >> RadioWrite
  - >> RadioSetTxConfig
  - >> RadioSetRxConfig
  - >> RadioSetPublicNetwork
  - >> RadioIrqProcess

  SX126xWriteRegisters (Thumb, 72 bytes, Stack size 24 bytes, radio.o(i.SX126xWriteRegisters))
  [Stack]

  - Max Depth = 192 + Unknown Stack Size
  - Call Chain = SX126xWriteRegisters ⇒ SX126xCheckDeviceReady ⇒ SX126xWakeup ⇒ SX126xWaitOnBusy ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SX126xCheckDeviceReady
  - >> SX126xWaitOnBusy
  - >> SX126xSpiInOut
  - >> SX126xSetNss
  [Called By]
  - >> SX126xSetSyncWord
  - >> SX126xWriteRegister
  - >> RadioWriteBuffer
  - >> SX126xSetCrcSeed
  - >> SX126xSetCrcPolynomial

  Spi1Init (Thumb, 162 bytes, Stack size 32 bytes, hal_spi.o(i.Spi1Init))
  [Stack]

  - Max Depth = 56
  - Call Chain = Spi1Init ⇒ GPIO_Init
  [Calls]
  - >> SPI_Init
  - >> SPI_Cmd
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_SetBits
  - >> GPIO_Init
  [Called By]
  - >> SX126xIoInit

  SysInit (Thumb, 158 bytes, Stack size 16 bytes, main.o(i.SysInit))
  [Stack]

  - Max Depth = 116
  - Call Chain = SysInit ⇒ HALUart1Init ⇒ USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> RCC_APB2PeriphClockCmd
  - >> NVIC_PriorityGroupConfig
  - >> HALUart1Init
  - >> GPIO_SetBits
  - >> GPIO_PinRemapConfig
  - >> GPIO_Init
  [Called By]
  - >> main

  SysTick_Handler (Thumb, 12 bytes, Stack size 0 bytes, stm32f10x_it.o(i.SysTick_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SystemInit (Thumb, 78 bytes, Stack size 8 bytes, system_stm32f10x.o(i.SystemInit))
  [Stack]

  - Max Depth = 28
  - Call Chain = SystemInit ⇒ SetSysClock ⇒ SetSysClockTo72
  [Calls]
  - >> SetSysClock
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(.text)

  TIM3_IRQHandler (Thumb, 176 bytes, Stack size 8 bytes, sx126xstm32f103-board.o(i.TIM3_IRQHandler))
  [Stack]

  - Max Depth = 160 + Unknown Stack Size
  - Call Chain = TIM3_IRQHandler ⇒ SX126xTxTimerStop ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> RadioOnTxTimeoutIrq
  - >> RadioOnRxTimeoutIrq
  - >> SX126xTxTimerStop
  - >> SX126xRxTimerStop
  - >> TIM_GetITStatus
  - >> TIM_ClearITPendingBit
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  TIM_ClearITPendingBit (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_tim.o(i.TIM_ClearITPendingBit))
  [Called By]

  - >> TIM3_IRQHandler
  - >> SX126xTimerInit

  TIM_Cmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_tim.o(i.TIM_Cmd))
  [Called By]

  - >> SX126xTimerInit

  TIM_GetITStatus (Thumb, 34 bytes, Stack size 12 bytes, stm32f10x_tim.o(i.TIM_GetITStatus))
  [Stack]

  - Max Depth = 12
  - Call Chain = TIM_GetITStatus
  [Called By]
  - >> TIM3_IRQHandler

  TIM_ITConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(i.TIM_ITConfig))
  [Called By]

  - >> SX126xTimerInit

  TIM_TimeBaseInit (Thumb, 122 bytes, Stack size 0 bytes, stm32f10x_tim.o(i.TIM_TimeBaseInit))
  [Called By]

  - >> SX126xTimerInit

  USART1_IRQHandler (Thumb, 40 bytes, Stack size 8 bytes, hal_uart.o(i.USART1_IRQHandler))
  [Stack]

  - Max Depth = 8
  - Call Chain = USART1_IRQHandler
  [Calls]
  - >> USART_SendData
  - >> USART_ReceiveData
  - >> USART_GetFlagStatus
  - >> USART_ClearFlag
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  USART_ClearFlag (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_usart.o(i.USART_ClearFlag))
  [Called By]

  - >> USART1_IRQHandler

  USART_Cmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(i.USART_Cmd))
  [Called By]

  - >> HALUart1Init

  USART_DeInit (Thumb, 134 bytes, Stack size 8 bytes, stm32f10x_usart.o(i.USART_DeInit))
  [Stack]

  - Max Depth = 8
  - Call Chain = USART_DeInit
  [Calls]
  - >> RCC_APB1PeriphResetCmd
  - >> RCC_APB2PeriphResetCmd
  [Called By]
  - >> HALUart1Init

  USART_GetFlagStatus (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_usart.o(i.USART_GetFlagStatus))
  [Called By]

  - >> fputc
  - >> USART1_IRQHandler

  USART_ITConfig (Thumb, 74 bytes, Stack size 20 bytes, stm32f10x_usart.o(i.USART_ITConfig))
  [Stack]

  - Max Depth = 20
  - Call Chain = USART_ITConfig
  [Called By]
  - >> HALUart1Init

  USART_Init (Thumb, 210 bytes, Stack size 56 bytes, stm32f10x_usart.o(i.USART_Init))
  [Stack]

  - Max Depth = 68
  - Call Chain = USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> RCC_GetClocksFreq
  [Called By]
  - >> HALUart1Init

  USART_ReceiveData (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_usart.o(i.USART_ReceiveData))
  [Called By]

  - >> USART1_IRQHandler

  USART_SendData (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_usart.o(i.USART_SendData))
  [Called By]

  - >> fputc
  - >> USART1_IRQHandler

  UsageFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(i.UsageFault_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  _is_digit (Thumb, 14 bytes, Stack size 0 bytes, __printf_wp.o(i._is_digit))
  [Called By]

  - >> __printf

  _sys_exit (Thumb, 4 bytes, Stack size 0 bytes, hal_uart.o(i._sys_exit))
  [Called By]

  - >> __rt_exit_exit

  delay_ms (Thumb, 18 bytes, Stack size 8 bytes, delay.o(i.delay_ms))
  [Stack]

  - Max Depth = 8
  - Call Chain = delay_ms
  [Calls]
  - >> delay_us
  [Called By]
  - >> ExampleSX126xSendDemo
  - >> main
  - >> SX126xDelayMs

  delay_us (Thumb, 26 bytes, Stack size 0 bytes, delay.o(i.delay_us))
  [Called By]

  - >> delay_ms

  fputc (Thumb, 32 bytes, Stack size 16 bytes, hal_uart.o(i.fputc))
  [Stack]

  - Max Depth = 16
  - Call Chain = fputc
  [Calls]
  - >> USART_SendData
  - >> USART_GetFlagStatus
  [Address Reference Count : 1]
  - _printf_char_file.o(.text)

  main (Thumb, 70 bytes, Stack size 0 bytes, main.o(i.main))
  [Stack]

  - Max Depth = 184 + Unknown Stack Size
  - Call Chain = main ⇒ ExampleSX126xSendDemo ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> delay_ms
  - >> Get_SysTick
  - >> GPIO_SetBits
  - >> GPIO_ResetBits
  - >> ExampleSX126xSendDemo
  - >> SysInit
  - >> __2printf
  [Called By]
  - >> __rt_entry_main

  ### Local Symbols

  SetSysClock (Thumb, 8 bytes, Stack size 8 bytes, system_stm32f10x.o(i.SetSysClock))
  [Stack]

  - Max Depth = 20
  - Call Chain = SetSysClock ⇒ SetSysClockTo72
  [Calls]
  - >> SetSysClockTo72
  [Called By]
  - >> SystemInit

  SetSysClockTo72 (Thumb, 214 bytes, Stack size 12 bytes, system_stm32f10x.o(i.SetSysClockTo72))
  [Stack]

  - Max Depth = 12
  - Call Chain = SetSysClockTo72
  [Called By]
  - >> SetSysClock

  RadioGetFskBandwidthRegValue (Thumb, 56 bytes, Stack size 0 bytes, radio.o(i.RadioGetFskBandwidthRegValue))
  [Called By]

  - >> RadioSetTxConfig
  - >> RadioSetRxConfig

  RadioGetGfskTimeOnAirNumerator (Thumb, 54 bytes, Stack size 24 bytes, radio.o(i.RadioGetGfskTimeOnAirNumerator))
  [Stack]

  - Max Depth = 24
  - Call Chain = RadioGetGfskTimeOnAirNumerator
  [Called By]
  - >> RadioTimeOnAir

  RadioGetLoRaBandwidthInHz (Thumb, 82 bytes, Stack size 0 bytes, radio.o(i.RadioGetLoRaBandwidthInHz))
  [Called By]

  - >> RadioTimeOnAir

  RadioGetLoRaTimeOnAirNumerator (Thumb, 178 bytes, Stack size 36 bytes, radio.o(i.RadioGetLoRaTimeOnAirNumerator))
  [Stack]

  - Max Depth = 36
  - Call Chain = RadioGetLoRaTimeOnAirNumerator
  [Called By]
  - >> RadioTimeOnAir

  SX126xConvertFreqInHzToPllStep (Thumb, 36 bytes, Stack size 8 bytes, sx126x.o(i.SX126xConvertFreqInHzToPllStep))
  [Stack]

  - Max Depth = 8
  - Call Chain = SX126xConvertFreqInHzToPllStep
  [Called By]
  - >> SX126xSetRfFrequency
  - >> SX126xSetModulationParams

  SX126xOnRxDone (Thumb, 44 bytes, Stack size 24 bytes, sx126x_example_send.o(i.SX126xOnRxDone))
  [Stack]

  - Max Depth = 168 + Unknown Stack Size
  - Call Chain = SX126xOnRxDone ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> __2printf
  [Address Reference Count : 1]
  - sx126x_example_send.o(i.ExampleSX126xSendDemo)

  SX126xOnRxError (Thumb, 26 bytes, Stack size 8 bytes, sx126x_example_send.o(i.SX126xOnRxError))
  [Stack]

  - Max Depth = 152 + Unknown Stack Size
  - Call Chain = SX126xOnRxError ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> __2printf
  [Address Reference Count : 1]
  - sx126x_example_send.o(i.ExampleSX126xSendDemo)

  SX126xOnRxTimeout (Thumb, 26 bytes, Stack size 8 bytes, sx126x_example_send.o(i.SX126xOnRxTimeout))
  [Stack]

  - Max Depth = 152 + Unknown Stack Size
  - Call Chain = SX126xOnRxTimeout ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> __2printf
  [Address Reference Count : 1]
  - sx126x_example_send.o(i.ExampleSX126xSendDemo)

  SX126xOnTxDone (Thumb, 16 bytes, Stack size 8 bytes, sx126x_example_send.o(i.SX126xOnTxDone))
  [Stack]

  - Max Depth = 152 + Unknown Stack Size
  - Call Chain = SX126xOnTxDone ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> __2printf
  [Address Reference Count : 1]
  - sx126x_example_send.o(i.ExampleSX126xSendDemo)

  SX126xOnTxTimeout (Thumb, 10 bytes, Stack size 8 bytes, sx126x_example_send.o(i.SX126xOnTxTimeout))
  [Stack]

  - Max Depth = 152 + Unknown Stack Size
  - Call Chain = SX126xOnTxTimeout ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> __2printf
  [Address Reference Count : 1]
  - sx126x_example_send.o(i.ExampleSX126xSendDemo)

  _printf_input_char (Thumb, 10 bytes, Stack size 0 bytes, _printf_char_common.o(.text))
  [Address Reference Count : 1]

  - _printf_char_common.o(.text)

  ### Undefined Global Symbols