# Static Call Graph for image .\STM3210E-EVAL\STM3210E-EVAL.axf

#<CALLGRAPH># ARM Linker, 5050106: Last Updated: Thu Jun 18 10:15:12 2020

### Maximum Stack Usage = 1096 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

USART1_IRQHandler ⇒ at_cmd_recv ⇒ at_cmd_parse ⇒ __2printf

### Mutually Recursive functions

- ADC1_2_IRQHandler ⇒ ADC1_2_IRQHandler
- BusFault_Handler ⇒ BusFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- UsageFault_Handler ⇒ UsageFault_Handler

  ### Function Pointers

  - ADC1_2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - ADC3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - AT_CmdFunc_ANCHOR_GPIOTEST from stm32_eval.o(i.AT_CmdFunc_ANCHOR_GPIOTEST) referenced 2 times from stm32_eval.o(.data)
  - AT_CmdFunc_ANCHOR_TAG from stm32_eval.o(i.AT_CmdFunc_ANCHOR_TAG) referenced 2 times from stm32_eval.o(.data)
  - AT_CmdFunc_AT from stm32_eval.o(i.AT_CmdFunc_AT) referenced 2 times from stm32_eval.o(.data)
  - AT_CmdFunc_FACTORY from stm32_eval.o(i.AT_CmdFunc_FACTORY) referenced 2 times from stm32_eval.o(.data)
  - AT_CmdFunc_RST from stm32_eval.o(i.AT_CmdFunc_RST) referenced 2 times from stm32_eval.o(.data)
  - AT_CmdFunc_TemHum from stm32_eval.o(i.AT_CmdFunc_TemHum) referenced 2 times from stm32_eval.o(.data)
  - AT_CmdFunc_XYZ from stm32_eval.o(i.AT_CmdFunc_XYZ) referenced 2 times from stm32_eval.o(.data)
  - AT_CmdFunc_interval from stm32_eval.o(i.AT_CmdFunc_interval) referenced 2 times from stm32_eval.o(.data)
  - AT_CmdFunc_ondis from stm32_eval.o(i.AT_CmdFunc_ondis) referenced 2 times from stm32_eval.o(.data)
  - AT_CmdFunc_version from stm32_eval.o(i.AT_CmdFunc_version) referenced 2 times from stm32_eval.o(.data)
  - BusFault_Handler from stm32f10x_it.o(i.BusFault_Handler) referenced from startup_stm32f10x_hd.o(RESET)
  - CAN1_RX1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - CAN1_SCE_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel4_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel6_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel7_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel4_5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DebugMon_Handler from stm32f10x_it.o(i.DebugMon_Handler) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI0_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI15_10_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI4_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI9_5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - FLASH_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - FSMC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - HardFault_Handler from stm32f10x_it.o(i.HardFault_Handler) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - MemManage_Handler from stm32f10x_it.o(i.MemManage_Handler) referenced from startup_stm32f10x_hd.o(RESET)
  - NMI_Handler from stm32f10x_it.o(i.NMI_Handler) referenced from startup_stm32f10x_hd.o(RESET)
  - PVD_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - PendSV_Handler from stm32f10x_it.o(i.PendSV_Handler) referenced from startup_stm32f10x_hd.o(RESET)
  - RCC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - RTCAlarm_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - RTC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - Reset_Handler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SDIO_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SPI1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SPI2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SPI3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SVC_Handler from stm32f10x_it.o(i.SVC_Handler) referenced from startup_stm32f10x_hd.o(RESET)
  - SysTick_Handler from stm32f10x_it.o(i.SysTick_Handler) referenced from startup_stm32f10x_hd.o(RESET)
  - SystemInit from system_stm32f10x.o(i.SystemInit) referenced from startup_stm32f10x_hd.o(.text)
  - TAMPER_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_BRK_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_TRG_COM_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_UP_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM4_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM6_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM7_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_BRK_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_CC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_TRG_COM_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_UP_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - UART4_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - UART5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USART1_IRQHandler from stm32_eval.o(i.USART1_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - USART2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USART3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USBWakeUp_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USB_HP_CAN1_TX_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USB_LP_CAN1_RX0_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - UsageFault_Handler from stm32f10x_it.o(i.UsageFault_Handler) referenced from startup_stm32f10x_hd.o(RESET)
  - WWDG_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_stm32f10x_hd.o(.text)
  - _sputc from printfa.o(i._sputc) referenced from printfa.o(i.__0sprintf)
  - fputc from main.o(i.fputc) referenced from printfa.o(i.__0printf)
  - main from main.o(i.main) referenced from entry9a.o(.ARM.Collect$$$$0000000B)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_cpp_init (Thumb, 0 bytes, Stack size unknown bytes, entry8b.o(.ARM.Collect$$$$0000000A))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry9a.o(.ARM.Collect$$$$0000000B))

  __rt_final_cpp (Thumb, 0 bytes, Stack size unknown bytes, entry10a.o(.ARM.Collect$$$$0000000D))

  __rt_final_exit (Thumb, 0 bytes, Stack size unknown bytes, entry11a.o(.ARM.Collect$$$$0000000F))

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  ADC1_2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Calls]

  - >> ADC1_2_IRQHandler
  [Called By]
  - >> ADC1_2_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  ADC3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel4_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  FSMC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  RTCAlarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  RTC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SDIO_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SPI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TAMPER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  UART4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  UART5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USBWakeUp_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USB_HP_CAN1_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USB_LP_CAN1_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  __aeabi_memset (Thumb, 14 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)
  [Called By]

  - >> _memset$wrapper
  - >> __aeabi_memclr

  __aeabi_memset4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memset8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memclr (Thumb, 4 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memset

  __aeabi_memclr4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text))
  [Called By]

  - >> at_cmd_parse

  __aeabi_memclr8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  _memset$wrapper (Thumb, 18 bytes, Stack size 8 bytes, memseta.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memset

  strstr (Thumb, 36 bytes, Stack size 12 bytes, strstr.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = strstr
  [Called By]
  - >> at_cmd_parse

  strlen (Thumb, 14 bytes, Stack size 0 bytes, strlen.o(.text))
  [Called By]

  - >> at_cmd_parse

  memcmp (Thumb, 26 bytes, Stack size 12 bytes, memcmp.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = memcmp
  [Called By]
  - >> TAG_MEASURE
  - >> ANTHOR_MEASURE
  - >> Tag_Measure_Dis

  strtok (Thumb, 62 bytes, Stack size 16 bytes, strtok.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = strtok
  [Called By]
  - >> AT_CmdFunc_ondis
  - >> AT_CmdFunc_interval
  - >> AT_CmdFunc_ANCHOR_TAG

  atoi (Thumb, 26 bytes, Stack size 16 bytes, atoi.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = atoi ⇒ strtol ⇒ _strtoul
  [Calls]
  - >> strtol
  - >> __aeabi_errno_addr
  [Called By]
  - >> AT_CmdFunc_ondis
  - >> AT_CmdFunc_interval
  - >> AT_CmdFunc_ANCHOR_TAG

  __aeabi_fadd (Thumb, 164 bytes, Stack size 16 bytes, fadd.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = __aeabi_fadd ⇒ _float_epilogue
  [Calls]
  - >> _float_round
  - >> _float_epilogue
  [Called By]
  - >> __aeabi_fsub
  - >> __aeabi_frsub

  __aeabi_fsub (Thumb, 6 bytes, Stack size 0 bytes, fadd.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = __aeabi_fsub ⇒ __aeabi_fadd ⇒ _float_epilogue
  [Calls]
  - >> __aeabi_fadd
  [Called By]
  - >> drv_lis2dh12_get_angle

  __aeabi_frsub (Thumb, 6 bytes, Stack size 0 bytes, fadd.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_fadd

  __aeabi_fdiv (Thumb, 124 bytes, Stack size 8 bytes, fdiv.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = __aeabi_fdiv
  [Calls]
  - >> _float_round
  [Called By]
  - >> distance_mange
  - >> drv_lis2dh12_get_angle

  __aeabi_dadd (Thumb, 322 bytes, Stack size 48 bytes, dadd.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = __aeabi_dadd ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_lasr
  - >> __aeabi_llsl
  - >> _double_round
  - >> _double_epilogue
  [Called By]
  - >> ANTHOR_MEASURE
  - >> drv_lis2dh12_get_angle
  - >> __aeabi_drsub
  - >> __aeabi_dsub
  - >> pow
  - >> asin
  - >> __kernel_poly
  - >> __mathlib_dbl_infnan2
  - >> _fp_digits

  __aeabi_dsub (Thumb, 6 bytes, Stack size 0 bytes, dadd.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = __aeabi_dsub ⇒ __aeabi_dadd ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_dadd
  [Called By]
  - >> ANTHOR_MEASURE
  - >> SHT20_read_tem
  - >> SHT20_read_hum
  - >> pow
  - >> asin

  __aeabi_drsub (Thumb, 6 bytes, Stack size 0 bytes, dadd.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = __aeabi_drsub ⇒ __aeabi_dadd ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_dadd
  [Called By]
  - >> ANTHOR_MEASURE
  - >> pow
  - >> asin

  __aeabi_dmul (Thumb, 228 bytes, Stack size 48 bytes, dmul.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> _double_epilogue
  [Called By]
  - >> ANTHOR_MEASURE
  - >> drv_lis2dh12_get_angle
  - >> SHT20_read_tem
  - >> SHT20_read_hum
  - >> dwt_getrangebias
  - >> pow
  - >> asin
  - >> __kernel_poly
  - >> _fp_digits

  __aeabi_ddiv (Thumb, 222 bytes, Stack size 32 bytes, ddiv.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = __aeabi_ddiv ⇒ _double_round
  [Calls]
  - >> _double_round
  [Called By]
  - >> ANTHOR_MEASURE
  - >> drv_lis2dh12_get_angle
  - >> pow
  - >> asin
  - >> __mathlib_dbl_invalid
  - >> __mathlib_dbl_divzero
  - >> _fp_digits

  __ARM_scalbn (Thumb, 46 bytes, Stack size 16 bytes, dscalb.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = __ARM_scalbn
  [Called By]
  - >> drv_lis2dh12_get_angle
  - >> dwt_getrangebias
  - >> pow
  - >> asin
  - >> __mathlib_dbl_underflow
  - >> __mathlib_dbl_overflow
  - >> __mathlib_dbl_infnan

  scalbn (Thumb, 0 bytes, Stack size 16 bytes, dscalb.o(.text), UNUSED)

  __aeabi_i2f (Thumb, 18 bytes, Stack size 0 bytes, fflti.o(.text))
  [Stack]

  - Max Depth = 4
  - Call Chain = __aeabi_i2f ⇒ _float_epilogue
  [Calls]
  - >> _float_epilogue
  [Called By]
  - >> distance_mange
  - >> drv_lis2dh12_get_angle
  - >> dwt_getrangebias

  __aeabi_ui2f (Thumb, 10 bytes, Stack size 0 bytes, ffltui.o(.text))
  [Stack]

  - Max Depth = 4
  - Call Chain = __aeabi_ui2f ⇒ _float_epilogue
  [Calls]
  - >> _float_epilogue
  [Called By]
  - >> SHT20_read_tem
  - >> SHT20_read_hum

  __aeabi_i2d (Thumb, 34 bytes, Stack size 16 bytes, dflti.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = __aeabi_i2d ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> _double_epilogue
  [Called By]
  - >> pow

  __aeabi_ui2d (Thumb, 26 bytes, Stack size 16 bytes, dfltui.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = __aeabi_ui2d ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> _double_epilogue
  [Called By]
  - >> ANTHOR_MEASURE

  __aeabi_l2d (Thumb, 40 bytes, Stack size 24 bytes, dfltl.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = __aeabi_l2d ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> _double_epilogue
  [Called By]
  - >> ANTHOR_MEASURE

  __aeabi_f2iz (Thumb, 50 bytes, Stack size 0 bytes, ffixi.o(.text))
  [Called By]

  - >> drv_lis2dh12_get_angle

  __aeabi_d2iz (Thumb, 62 bytes, Stack size 16 bytes, dfixi.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = __aeabi_d2iz
  [Calls]
  - >> __aeabi_llsr
  [Called By]
  - >> ANTHOR_MEASURE
  - >> dwt_getrangebias

  __aeabi_d2lz (Thumb, 74 bytes, Stack size 16 bytes, dfixl.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = __aeabi_d2lz
  [Calls]
  - >> __aeabi_llsr
  - >> __aeabi_llsl
  [Called By]
  - >> ANTHOR_MEASURE

  __aeabi_f2d (Thumb, 38 bytes, Stack size 0 bytes, f2d.o(.text))
  [Called By]

  - >> distance_mange
  - >> drv_lis2dh12_get_angle
  - >> SHT20_read_tem
  - >> SHT20_read_hum
  - >> AT_CmdFunc_XYZ
  - >> AT_CmdFunc_TemHum
  - >> dwt_getrangebias

  __aeabi_cdrcmple (Thumb, 48 bytes, Stack size 0 bytes, cdrcmple.o(.text))
  [Called By]

  - >> pow
  - >> _fp_digits

  __aeabi_d2f (Thumb, 56 bytes, Stack size 8 bytes, d2f.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = __aeabi_d2f
  [Calls]
  - >> _float_round
  [Called By]
  - >> ANTHOR_MEASURE
  - >> drv_lis2dh12_get_angle
  - >> SHT20_read_tem
  - >> SHT20_read_hum

  __aeabi_cfrcmple (Thumb, 20 bytes, Stack size 0 bytes, cfrcmple.o(.text))
  [Called By]

  - >> drv_lis2dh12_get_angle

  __aeabi_uidiv (Thumb, 0 bytes, Stack size 12 bytes, uidiv.o(.text), UNUSED)

  __aeabi_uidivmod (Thumb, 44 bytes, Stack size 12 bytes, uidiv.o(.text), UNUSED)
  [Called By]

  - >> _printf_core

  __aeabi_uldivmod (Thumb, 98 bytes, Stack size 40 bytes, uldiv.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_llsr
  - >> __aeabi_llsl
  [Called By]
  - >> _printf_core
  - >> _fp_digits

  __aeabi_llsl (Thumb, 30 bytes, Stack size 0 bytes, llshl.o(.text))
  [Called By]

  - >> __aeabi_dadd
  - >> __aeabi_d2lz
  - >> __aeabi_uldivmod
  - >> _double_epilogue
  - >> __aeabi_d2ulz

  _ll_shift_l (Thumb, 0 bytes, Stack size 0 bytes, llshl.o(.text), UNUSED)

  __aeabi_llsr (Thumb, 32 bytes, Stack size 0 bytes, llushr.o(.text))
  [Called By]

  - >> __aeabi_d2iz
  - >> _dsqrt
  - >> __aeabi_d2lz
  - >> __aeabi_uldivmod
  - >> _double_epilogue
  - >> __aeabi_d2ulz

  _ll_ushift_r (Thumb, 0 bytes, Stack size 0 bytes, llushr.o(.text), UNUSED)

  __aeabi_lasr (Thumb, 36 bytes, Stack size 0 bytes, llsshr.o(.text))
  [Called By]

  - >> __aeabi_dadd

  _ll_sshift_r (Thumb, 0 bytes, Stack size 0 bytes, llsshr.o(.text), UNUSED)

  strtol (Thumb, 112 bytes, Stack size 32 bytes, strtol.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = strtol ⇒ _strtoul
  [Calls]
  - >> _strtoul
  - >> __rt_ctype_table
  - >> __aeabi_errno_addr
  [Called By]
  - >> atoi

  __I$use$fp (Thumb, 0 bytes, Stack size 0 bytes, iusefp.o(.text), UNUSED)

  _float_round (Thumb, 18 bytes, Stack size 0 bytes, fepilogue.o(.text))
  [Called By]

  - >> __aeabi_fdiv
  - >> __aeabi_fadd
  - >> __aeabi_d2f

  _float_epilogue (Thumb, 92 bytes, Stack size 4 bytes, fepilogue.o(.text))
  [Stack]

  - Max Depth = 4
  - Call Chain = _float_epilogue
  [Called By]
  - >> __aeabi_i2f
  - >> __aeabi_fadd
  - >> __aeabi_ui2f

  _double_round (Thumb, 30 bytes, Stack size 8 bytes, depilogue.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = _double_round
  [Called By]
  - >> __aeabi_ddiv
  - >> __aeabi_dadd
  - >> _dsqrt
  - >> _double_epilogue

  _double_epilogue (Thumb, 156 bytes, Stack size 32 bytes, depilogue.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_llsr
  - >> __aeabi_llsl
  - >> _double_round
  [Called By]
  - >> __aeabi_ui2d
  - >> __aeabi_i2d
  - >> __aeabi_dmul
  - >> __aeabi_dadd
  - >> __aeabi_l2d

  _dsqrt (Thumb, 162 bytes, Stack size 32 bytes, dsqrt.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = _dsqrt ⇒ _double_round
  [Calls]
  - >> __aeabi_llsr
  - >> _double_round
  [Called By]
  - >> sqrt

  __aeabi_d2ulz (Thumb, 48 bytes, Stack size 0 bytes, dfixul.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_llsr
  - >> __aeabi_llsl
  [Called By]
  - >> _fp_digits

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  __rt_ctype_table (Thumb, 4 bytes, Stack size 0 bytes, ctype_o.o(.text))
  [Called By]

  - >> strtol

  _strtoul (Thumb, 158 bytes, Stack size 40 bytes, _strtoul.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = _strtoul
  [Calls]
  - >> _chval
  - >> __aeabi_errno_addr
  [Called By]
  - >> strtol

  _chval (Thumb, 28 bytes, Stack size 0 bytes, _chval.o(.text))
  [Called By]

  - >> _strtoul

  __decompress (Thumb, 0 bytes, Stack size unknown bytes, __dczerorl2.o(.text), UNUSED)

  __decompress1 (Thumb, 86 bytes, Stack size unknown bytes, __dczerorl2.o(.text), UNUSED)

  ANTHOR_MEASURE (Thumb, 676 bytes, Stack size 64 bytes, lib.o(i.ANTHOR_MEASURE))
  [Stack]

  - Max Depth = 168
  - Call Chain = ANTHOR_MEASURE ⇒ dwt_starttx ⇒ dwt_entersleepaftertx ⇒ dwt_read32bitoffsetreg ⇒ dwt_readfromdevice ⇒ readfromspi_serial ⇒ decamutexon
  [Calls]
  - >> get_tx_timestamp_u64
  - >> get_rx_timestamp_u64
  - >> dwt_writetxfctrl
  - >> dwt_writetxdata
  - >> dwt_write32bitoffsetreg
  - >> dwt_starttx
  - >> dwt_setrxtimeout
  - >> dwt_setrxaftertxdelay
  - >> dwt_rxenable
  - >> dwt_readrxdata
  - >> dwt_read32bitoffsetreg
  - >> USART_puts
  - >> __aeabi_ui2d
  - >> __aeabi_drsub
  - >> __aeabi_d2iz
  - >> dwt_getrangebias
  - >> __aeabi_dsub
  - >> __aeabi_dmul
  - >> __aeabi_ddiv
  - >> __aeabi_dadd
  - >> __aeabi_d2f
  - >> memcmp
  - >> putc
  - >> __aeabi_l2d
  - >> __aeabi_d2lz
  - >> final_msg_get_ts
  [Called By]
  - >> main

  AT_CmdFunc_ANCHOR_GPIOTEST (Thumb, 30 bytes, Stack size 8 bytes, stm32_eval.o(i.AT_CmdFunc_ANCHOR_GPIOTEST))
  [Stack]

  - Max Depth = 120
  - Call Chain = AT_CmdFunc_ANCHOR_GPIOTEST ⇒ buo1Gpio ⇒ PairGpioCheck ⇒ dwt_getgpiovalue ⇒ dwt_read32bitoffsetreg ⇒ dwt_readfromdevice ⇒ readfromspi_serial ⇒ decamutexon
  [Calls]
  - >> buo1Gpio
  - >> buo1DbGpio
  [Address Reference Count : 1]
  - stm32_eval.o(.data)

  AT_CmdFunc_ANCHOR_TAG (Thumb, 158 bytes, Stack size 24 bytes, stm32_eval.o(i.AT_CmdFunc_ANCHOR_TAG))
  [Stack]

  - Max Depth = 112
  - Call Chain = AT_CmdFunc_ANCHOR_TAG ⇒ atoi ⇒ strtol ⇒ _strtoul
  [Calls]
  - >> FLASH_ReadMoreData
  - >> FLASH_WriteMoreData
  - >> strtok
  - >> atoi
  - >> __2printf
  [Address Reference Count : 1]
  - stm32_eval.o(.data)

  AT_CmdFunc_AT (Thumb, 4 bytes, Stack size 0 bytes, stm32_eval.o(i.AT_CmdFunc_AT))
  [Address Reference Count : 1]

  - stm32_eval.o(.data)

  AT_CmdFunc_FACTORY (Thumb, 30 bytes, Stack size 16 bytes, stm32_eval.o(i.AT_CmdFunc_FACTORY))
  [Stack]

  - Max Depth = 64
  - Call Chain = AT_CmdFunc_FACTORY ⇒ FLASH_WriteMoreData ⇒ FLASH_ProgramHalfWord ⇒ FLASH_WaitForLastOperation
  [Calls]
  - >> FLASH_WriteMoreData
  [Address Reference Count : 1]
  - stm32_eval.o(.data)

  AT_CmdFunc_RST (Thumb, 36 bytes, Stack size 8 bytes, stm32_eval.o(i.AT_CmdFunc_RST))
  [Stack]

  - Max Depth = 32
  - Call Chain = AT_CmdFunc_RST ⇒ __2printf
  [Calls]
  - >> __2printf
  [Address Reference Count : 1]
  - stm32_eval.o(.data)

  AT_CmdFunc_TemHum (Thumb, 60 bytes, Stack size 16 bytes, stm32_eval.o(i.AT_CmdFunc_TemHum))
  [Stack]

  - Max Depth = 136
  - Call Chain = AT_CmdFunc_TemHum ⇒ SHT20_read_tem ⇒ __aeabi_dsub ⇒ __aeabi_dadd ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_f2d
  - >> SHT20_read_tem
  - >> SHT20_read_hum
  - >> __2printf
  [Address Reference Count : 1]
  - stm32_eval.o(.data)

  AT_CmdFunc_XYZ (Thumb, 36 bytes, Stack size 8 bytes, stm32_eval.o(i.AT_CmdFunc_XYZ))
  [Stack]

  - Max Depth = 280
  - Call Chain = AT_CmdFunc_XYZ ⇒ drv_lis2dh12_get_angle ⇒ pow ⇒ __kernel_poly ⇒ __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_f2d
  - >> drv_lis2dh12_get_angle
  - >> __2printf
  [Address Reference Count : 1]
  - stm32_eval.o(.data)

  AT_CmdFunc_interval (Thumb, 44 bytes, Stack size 8 bytes, stm32_eval.o(i.AT_CmdFunc_interval))
  [Stack]

  - Max Depth = 96
  - Call Chain = AT_CmdFunc_interval ⇒ atoi ⇒ strtol ⇒ _strtoul
  [Calls]
  - >> strtok
  - >> atoi
  [Address Reference Count : 1]
  - stm32_eval.o(.data)

  AT_CmdFunc_ondis (Thumb, 44 bytes, Stack size 8 bytes, stm32_eval.o(i.AT_CmdFunc_ondis))
  [Stack]

  - Max Depth = 96
  - Call Chain = AT_CmdFunc_ondis ⇒ atoi ⇒ strtol ⇒ _strtoul
  [Calls]
  - >> strtok
  - >> atoi
  [Address Reference Count : 1]
  - stm32_eval.o(.data)

  AT_CmdFunc_version (Thumb, 24 bytes, Stack size 8 bytes, stm32_eval.o(i.AT_CmdFunc_version))
  [Stack]

  - Max Depth = 32
  - Call Chain = AT_CmdFunc_version ⇒ __2printf
  [Calls]
  - >> __2printf
  [Address Reference Count : 1]
  - stm32_eval.o(.data)

  Anchor_Array_Init (Thumb, 28 bytes, Stack size 0 bytes, main.o(i.Anchor_Array_Init))
  [Called By]

  - >> main

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.BusFault_Handler))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.DebugMon_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI_GetITEnStatus (Thumb, 16 bytes, Stack size 0 bytes, port.o(i.EXTI_GetITEnStatus))
  [Called By]

  - >> decamutexon

  FLASH_ErasePage (Thumb, 56 bytes, Stack size 16 bytes, stm32f10x_flash.o(i.FLASH_ErasePage))
  [Stack]

  - Max Depth = 20
  - Call Chain = FLASH_ErasePage ⇒ FLASH_WaitForLastOperation
  [Calls]
  - >> FLASH_WaitForLastOperation
  [Called By]
  - >> FLASH_WriteMoreData

  FLASH_GetBank1Status (Thumb, 34 bytes, Stack size 0 bytes, stm32f10x_flash.o(i.FLASH_GetBank1Status))
  [Called By]

  - >> FLASH_WaitForLastOperation

  FLASH_Lock (Thumb, 12 bytes, Stack size 0 bytes, stm32f10x_flash.o(i.FLASH_Lock))
  [Called By]

  - >> FLASH_WriteMoreData

  FLASH_ProgramHalfWord (Thumb, 48 bytes, Stack size 20 bytes, stm32f10x_flash.o(i.FLASH_ProgramHalfWord))
  [Stack]

  - Max Depth = 24
  - Call Chain = FLASH_ProgramHalfWord ⇒ FLASH_WaitForLastOperation
  [Calls]
  - >> FLASH_WaitForLastOperation
  [Called By]
  - >> FLASH_WriteMoreData

  FLASH_ReadMoreData (Thumb, 26 bytes, Stack size 8 bytes, stm32_eval.o(i.FLASH_ReadMoreData))
  [Stack]

  - Max Depth = 8
  - Call Chain = FLASH_ReadMoreData
  [Called By]
  - >> main
  - >> AT_CmdFunc_ANCHOR_TAG

  FLASH_Unlock (Thumb, 12 bytes, Stack size 0 bytes, stm32f10x_flash.o(i.FLASH_Unlock))
  [Called By]

  - >> FLASH_WriteMoreData

  FLASH_WaitForLastOperation (Thumb, 36 bytes, Stack size 4 bytes, stm32f10x_flash.o(i.FLASH_WaitForLastOperation))
  [Stack]

  - Max Depth = 4
  - Call Chain = FLASH_WaitForLastOperation
  [Calls]
  - >> FLASH_GetBank1Status
  [Called By]
  - >> FLASH_ProgramHalfWord
  - >> FLASH_ErasePage

  FLASH_WriteMoreData (Thumb, 84 bytes, Stack size 24 bytes, stm32_eval.o(i.FLASH_WriteMoreData))
  [Stack]

  - Max Depth = 48
  - Call Chain = FLASH_WriteMoreData ⇒ FLASH_ProgramHalfWord ⇒ FLASH_WaitForLastOperation
  [Calls]
  - >> FLASH_Unlock
  - >> FLASH_ProgramHalfWord
  - >> FLASH_Lock
  - >> FLASH_ErasePage
  [Called By]
  - >> AT_CmdFunc_FACTORY
  - >> AT_CmdFunc_ANCHOR_TAG

  GPIO_Configuration (Thumb, 216 bytes, Stack size 24 bytes, port.o(i.GPIO_Configuration))
  [Stack]

  - Max Depth = 44
  - Call Chain = GPIO_Configuration ⇒ GPIO_PinRemapConfig
  [Calls]
  - >> GPIO_PinRemapConfig
  - >> GPIO_Init
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_SetBits
  [Called By]
  - >> peripherals_init

  GPIO_Init (Thumb, 162 bytes, Stack size 20 bytes, stm32f10x_gpio.o(i.GPIO_Init))
  [Stack]

  - Max Depth = 20
  - Call Chain = GPIO_Init
  [Called By]
  - >> reset_DW1000
  - >> STM_EVAL_COMInit
  - >> PairGpioCheckDB
  - >> SPI_Configuration
  - >> GPIO_Configuration
  - >> MX_I2C1_Init

  GPIO_PinRemapConfig (Thumb, 82 bytes, Stack size 20 bytes, stm32f10x_gpio.o(i.GPIO_PinRemapConfig))
  [Stack]

  - Max Depth = 20
  - Call Chain = GPIO_PinRemapConfig
  [Called By]
  - >> buo1DbGpio
  - >> GPIO_Configuration

  GPIO_ReadInputDataBit (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_gpio.o(i.GPIO_ReadInputDataBit))
  [Called By]

  - >> PairGpioCheckDB

  GPIO_ResetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_gpio.o(i.GPIO_ResetBits))
  [Called By]

  - >> reset_DW1000
  - >> TAG_MEASURE
  - >> main
  - >> PairGpioCheckDB

  GPIO_SetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_gpio.o(i.GPIO_SetBits))
  [Called By]

  - >> TAG_MEASURE
  - >> main
  - >> Tag_Measure_Dis
  - >> PairGpioCheckDB
  - >> SPI_Configuration
  - >> GPIO_Configuration

  HardFault_Handler (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_it.o(i.HardFault_Handler))
  [Stack]

  - Max Depth = 24
  - Call Chain = HardFault_Handler ⇒ __2printf
  [Calls]
  - >> __2printf
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  I2C_AcknowledgeConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_i2c.o(i.I2C_AcknowledgeConfig))
  [Called By]

  - >> MX_I2C1_Init
  - >> hal_i2c1_send_data1
  - >> hal_i2c1_read_data
  - >> drv_lis2dh12_iic_read_byte
  - >> I2C_WriteOneByte

  I2C_CheckEvent (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_i2c.o(i.I2C_CheckEvent))
  [Called By]

  - >> hal_i2c1_send_data1
  - >> hal_i2c1_read_data
  - >> drv_lis2dh12_iic_read_byte
  - >> I2C_WriteOneByte

  I2C_Cmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_i2c.o(i.I2C_Cmd))
  [Called By]

  - >> MX_I2C1_Init

  I2C_DeInit (Thumb, 38 bytes, Stack size 8 bytes, stm32f10x_i2c.o(i.I2C_DeInit))
  [Stack]

  - Max Depth = 8
  - Call Chain = I2C_DeInit
  [Calls]
  - >> RCC_APB1PeriphResetCmd
  [Called By]
  - >> MX_I2C1_Init

  I2C_GenerateSTART (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_i2c.o(i.I2C_GenerateSTART))
  [Called By]

  - >> hal_i2c1_send_data1
  - >> hal_i2c1_read_data
  - >> drv_lis2dh12_iic_read_byte
  - >> I2C_WriteOneByte

  I2C_GenerateSTOP (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_i2c.o(i.I2C_GenerateSTOP))
  [Called By]

  - >> hal_i2c1_send_data1
  - >> hal_i2c1_read_data
  - >> drv_lis2dh12_iic_read_byte
  - >> I2C_WriteOneByte

  I2C_GetFlagStatus (Thumb, 42 bytes, Stack size 12 bytes, stm32f10x_i2c.o(i.I2C_GetFlagStatus))
  [Stack]

  - Max Depth = 12
  - Call Chain = I2C_GetFlagStatus
  [Called By]
  - >> hal_i2c1_send_data1
  - >> hal_i2c1_read_data
  - >> drv_lis2dh12_iic_read_byte
  - >> I2C_WriteOneByte

  I2C_Init (Thumb, 178 bytes, Stack size 40 bytes, stm32f10x_i2c.o(i.I2C_Init))
  [Stack]

  - Max Depth = 52
  - Call Chain = I2C_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> RCC_GetClocksFreq
  [Called By]
  - >> MX_I2C1_Init

  I2C_NACKPositionConfig (Thumb, 22 bytes, Stack size 0 bytes, stm32f10x_i2c.o(i.I2C_NACKPositionConfig))
  [Called By]

  - >> hal_i2c1_read_data
  - >> drv_lis2dh12_iic_read_byte

  I2C_ReceiveData (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_i2c.o(i.I2C_ReceiveData))
  [Called By]

  - >> hal_i2c1_read_data
  - >> drv_lis2dh12_iic_read_byte

  I2C_Send7bitAddress (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_i2c.o(i.I2C_Send7bitAddress))
  [Called By]

  - >> hal_i2c1_send_data1
  - >> hal_i2c1_read_data
  - >> drv_lis2dh12_iic_read_byte
  - >> I2C_WriteOneByte

  I2C_SendData (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_i2c.o(i.I2C_SendData))
  [Called By]

  - >> hal_i2c1_send_data1
  - >> drv_lis2dh12_iic_read_byte
  - >> I2C_WriteOneByte

  I2C_WriteOneByte (Thumb, 182 bytes, Stack size 32 bytes, lcd_oled.o(i.I2C_WriteOneByte))
  [Stack]

  - Max Depth = 44
  - Call Chain = I2C_WriteOneByte ⇒ I2C_GetFlagStatus
  [Calls]
  - >> I2C_SendData
  - >> I2C_Send7bitAddress
  - >> I2C_GetFlagStatus
  - >> I2C_GenerateSTOP
  - >> I2C_GenerateSTART
  - >> I2C_CheckEvent
  - >> I2C_AcknowledgeConfig
  [Called By]
  - >> SHT20_init
  - >> drv_lis2dh12_iic_write_byte
  - >> OLED_WR_Byte

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.MemManage_Handler))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.NMI_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  NVIC_Init (Thumb, 94 bytes, Stack size 16 bytes, misc.o(i.NVIC_Init))
  [Stack]

  - Max Depth = 16
  - Call Chain = NVIC_Init
  [Called By]
  - >> STM_EVAL_COMInit

  NVIC_PriorityGroupConfig (Thumb, 10 bytes, Stack size 0 bytes, misc.o(i.NVIC_PriorityGroupConfig))
  [Called By]

  - >> STM_EVAL_COMInit

  OLED_Clear (Thumb, 60 bytes, Stack size 16 bytes, lcd_oled.o(i.OLED_Clear))
  [Stack]

  - Max Depth = 68
  - Call Chain = OLED_Clear ⇒ OLED_WR_Byte ⇒ I2C_WriteOneByte ⇒ I2C_GetFlagStatus
  [Calls]
  - >> OLED_WR_Byte
  [Called By]
  - >> peripherals_init
  - >> OLED_Init

  OLED_Init (Thumb, 250 bytes, Stack size 8 bytes, lcd_oled.o(i.OLED_Init))
  [Stack]

  - Max Depth = 76
  - Call Chain = OLED_Init ⇒ OLED_Clear ⇒ OLED_WR_Byte ⇒ I2C_WriteOneByte ⇒ I2C_GetFlagStatus
  [Calls]
  - >> OLED_Clear
  - >> OLED_WR_Byte
  [Called By]
  - >> peripherals_init

  OLED_Set_Pos (Thumb, 44 bytes, Stack size 8 bytes, lcd_oled.o(i.OLED_Set_Pos))
  [Stack]

  - Max Depth = 60
  - Call Chain = OLED_Set_Pos ⇒ OLED_WR_Byte ⇒ I2C_WriteOneByte ⇒ I2C_GetFlagStatus
  [Calls]
  - >> OLED_WR_Byte
  [Called By]
  - >> OLED_ShowChar

  OLED_ShowChar (Thumb, 94 bytes, Stack size 24 bytes, lcd_oled.o(i.OLED_ShowChar))
  [Stack]

  - Max Depth = 84
  - Call Chain = OLED_ShowChar ⇒ OLED_Set_Pos ⇒ OLED_WR_Byte ⇒ I2C_WriteOneByte ⇒ I2C_GetFlagStatus
  [Calls]
  - >> OLED_WR_Byte
  - >> OLED_Set_Pos
  [Called By]
  - >> OLED_ShowString

  OLED_ShowString (Thumb, 50 bytes, Stack size 24 bytes, lcd_oled.o(i.OLED_ShowString))
  [Stack]

  - Max Depth = 108
  - Call Chain = OLED_ShowString ⇒ OLED_ShowChar ⇒ OLED_Set_Pos ⇒ OLED_WR_Byte ⇒ I2C_WriteOneByte ⇒ I2C_GetFlagStatus
  [Calls]
  - >> OLED_ShowChar
  [Called By]
  - >> main
  - >> distance_mange

  OLED_WR_Byte (Thumb, 36 bytes, Stack size 8 bytes, lcd_oled.o(i.OLED_WR_Byte))
  [Stack]

  - Max Depth = 52
  - Call Chain = OLED_WR_Byte ⇒ I2C_WriteOneByte ⇒ I2C_GetFlagStatus
  [Calls]
  - >> I2C_WriteOneByte
  [Called By]
  - >> OLED_Init
  - >> OLED_Clear
  - >> OLED_ShowChar
  - >> OLED_Set_Pos

  PairGpioCheck (Thumb, 132 bytes, Stack size 24 bytes, stm32_eval.o(i.PairGpioCheck))
  [Stack]

  - Max Depth = 104
  - Call Chain = PairGpioCheck ⇒ dwt_getgpiovalue ⇒ dwt_read32bitoffsetreg ⇒ dwt_readfromdevice ⇒ readfromspi_serial ⇒ decamutexon
  [Calls]
  - >> dwt_setGPIOvalue
  - >> dwt_setGPIOdirection
  - >> dwt_getgpiovalue
  [Called By]
  - >> buo1Gpio

  PairGpioCheckDB (Thumb, 194 bytes, Stack size 40 bytes, stm32_eval.o(i.PairGpioCheckDB))
  [Stack]

  - Max Depth = 60
  - Call Chain = PairGpioCheckDB ⇒ GPIO_Init
  [Calls]
  - >> GPIO_ReadInputDataBit
  - >> GPIO_Init
  - >> GPIO_SetBits
  - >> GPIO_ResetBits
  [Called By]
  - >> buo1DbGpio

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.PendSV_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  RCC_APB1PeriphClockCmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_APB1PeriphClockCmd))
  [Called By]

  - >> peripherals_init
  - >> STM_EVAL_COMInit
  - >> MX_I2C1_Init

  RCC_APB1PeriphResetCmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_APB1PeriphResetCmd))
  [Called By]

  - >> SPI_I2S_DeInit
  - >> I2C_DeInit

  RCC_APB2PeriphClockCmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_APB2PeriphClockCmd))
  [Called By]

  - >> peripherals_init
  - >> buo1DbGpio
  - >> STM_EVAL_COMInit
  - >> GPIO_Configuration
  - >> MX_I2C1_Init

  RCC_APB2PeriphResetCmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_APB2PeriphResetCmd))
  [Called By]

  - >> SPI_I2S_DeInit

  RCC_GetClocksFreq (Thumb, 140 bytes, Stack size 12 bytes, stm32f10x_rcc.o(i.RCC_GetClocksFreq))
  [Stack]

  - Max Depth = 12
  - Call Chain = RCC_GetClocksFreq
  [Called By]
  - >> USART_Init
  - >> I2C_Init

  SHT20_init (Thumb, 112 bytes, Stack size 24 bytes, lcd_oled.o(i.SHT20_init))
  [Stack]

  - Max Depth = 92
  - Call Chain = SHT20_init ⇒ hal_i2c1_send_data ⇒ hal_i2c1_send_data1 ⇒ I2C_GetFlagStatus
  [Calls]
  - >> hal_i2c1_send_data
  - >> hal_i2c1_read_data
  - >> I2C_WriteOneByte
  [Called By]
  - >> peripherals_init

  SHT20_read_hum (Thumb, 138 bytes, Stack size 32 bytes, lcd_oled.o(i.SHT20_read_hum))
  [Stack]

  - Max Depth = 120
  - Call Chain = SHT20_read_hum ⇒ __aeabi_dsub ⇒ __aeabi_dadd ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_f2d
  - >> __aeabi_ui2f
  - >> __aeabi_dsub
  - >> __aeabi_dmul
  - >> __aeabi_d2f
  - >> hal_i2c1_send_data
  - >> hal_i2c1_read_data
  - >> printf
  [Called By]
  - >> AT_CmdFunc_TemHum

  SHT20_read_tem (Thumb, 136 bytes, Stack size 32 bytes, lcd_oled.o(i.SHT20_read_tem))
  [Stack]

  - Max Depth = 120
  - Call Chain = SHT20_read_tem ⇒ __aeabi_dsub ⇒ __aeabi_dadd ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_f2d
  - >> __aeabi_ui2f
  - >> __aeabi_dsub
  - >> __aeabi_dmul
  - >> __aeabi_d2f
  - >> hal_i2c1_send_data
  - >> hal_i2c1_read_data
  - >> __2printf
  [Called By]
  - >> AT_CmdFunc_TemHum

  SPI_ChangeRate (Thumb, 14 bytes, Stack size 0 bytes, port.o(i.SPI_ChangeRate))
  [Called By]

  - >> spi_set_rate_low
  - >> spi_set_rate_high

  SPI_Cmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_spi.o(i.SPI_Cmd))
  [Called By]

  - >> SPI_Configuration

  SPI_Configuration (Thumb, 166 bytes, Stack size 48 bytes, port.o(i.SPI_Configuration))
  [Stack]

  - Max Depth = 68
  - Call Chain = SPI_Configuration ⇒ GPIO_Init
  [Calls]
  - >> GPIO_Init
  - >> GPIO_SetBits
  - >> SPI_SSOutputCmd
  - >> SPI_Init
  - >> SPI_I2S_DeInit
  - >> SPI_Cmd
  [Called By]
  - >> peripherals_init

  SPI_I2S_DeInit (Thumb, 72 bytes, Stack size 8 bytes, stm32f10x_spi.o(i.SPI_I2S_DeInit))
  [Stack]

  - Max Depth = 8
  - Call Chain = SPI_I2S_DeInit
  [Calls]
  - >> RCC_APB2PeriphResetCmd
  - >> RCC_APB1PeriphResetCmd
  [Called By]
  - >> SPI_Configuration

  SPI_I2S_GetFlagStatus (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_spi.o(i.SPI_I2S_GetFlagStatus))
  [Called By]

  - >> readfromspi_serial

  SPI_Init (Thumb, 56 bytes, Stack size 12 bytes, stm32f10x_spi.o(i.SPI_Init))
  [Stack]

  - Max Depth = 12
  - Call Chain = SPI_Init
  [Called By]
  - >> SPI_Configuration

  SPI_SSOutputCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_spi.o(i.SPI_SSOutputCmd))
  [Called By]

  - >> SPI_Configuration

  STM_EVAL_COMInit (Thumb, 200 bytes, Stack size 24 bytes, stm32_eval.o(i.STM_EVAL_COMInit))
  [Stack]

  - Max Depth = 68
  - Call Chain = STM_EVAL_COMInit ⇒ USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> NVIC_PriorityGroupConfig
  - >> NVIC_Init
  - >> GPIO_Init
  - >> RCC_APB2PeriphClockCmd
  - >> RCC_APB1PeriphClockCmd
  - >> USART_Init
  - >> USART_ITConfig
  - >> USART_Cmd
  [Called By]
  - >> usartinit

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.SVC_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  Semaphore_Init (Thumb, 8 bytes, Stack size 0 bytes, main.o(i.Semaphore_Init))
  [Called By]

  - >> main

  Sum_Tag_Semaphore_request (Thumb, 22 bytes, Stack size 0 bytes, main.o(i.Sum_Tag_Semaphore_request))
  [Called By]

  - >> TAG_MEASURE

  SysTick_Configuration (Thumb, 64 bytes, Stack size 16 bytes, port.o(i.SysTick_Configuration))
  [Stack]

  - Max Depth = 16
  - Call Chain = SysTick_Configuration
  [Calls]
  - >> NVIC_SetPriority
  [Called By]
  - >> peripherals_init

  SysTick_Handler (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_it.o(i.SysTick_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SystemInit (Thumb, 64 bytes, Stack size 8 bytes, system_stm32f10x.o(i.SystemInit))
  [Stack]

  - Max Depth = 20
  - Call Chain = SystemInit ⇒ SetSysClockTo72
  [Calls]
  - >> SetSysClockTo72
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(.text)

  TAG_MEASURE (Thumb, 1070 bytes, Stack size 0 bytes, lib.o(i.TAG_MEASURE))
  [Stack]

  - Max Depth = 200
  - Call Chain = TAG_MEASURE ⇒ Tag_Measure_Dis ⇒ distance_mange ⇒ compute_angle_send_to_anthor0 ⇒ dwt_starttx ⇒ dwt_entersleepaftertx ⇒ dwt_read32bitoffsetreg ⇒ dwt_readfromdevice ⇒ readfromspi_serial ⇒ decamutexon
  [Calls]
  - >> portGetTickCnt
  - >> dwt_writetxfctrl
  - >> dwt_writetxdata
  - >> dwt_write32bitoffsetreg
  - >> dwt_starttx
  - >> dwt_setrxtimeout
  - >> dwt_setrxaftertxdelay
  - >> dwt_rxenable
  - >> dwt_readrxdata
  - >> dwt_read32bitoffsetreg
  - >> GPIO_SetBits
  - >> GPIO_ResetBits
  - >> Tag_Measure_Dis
  - >> Sum_Tag_Semaphore_request
  - >> memcmp
  - >> NVIC_SystemReset
  [Called By]
  - >> main

  Tag_Measure_Dis (Thumb, 566 bytes, Stack size 40 bytes, main.o(i.Tag_Measure_Dis))
  [Stack]

  - Max Depth = 200
  - Call Chain = Tag_Measure_Dis ⇒ distance_mange ⇒ compute_angle_send_to_anthor0 ⇒ dwt_starttx ⇒ dwt_entersleepaftertx ⇒ dwt_read32bitoffsetreg ⇒ dwt_readfromdevice ⇒ readfromspi_serial ⇒ decamutexon
  [Calls]
  - >> portGetTickCnt
  - >> get_tx_timestamp_u64
  - >> get_rx_timestamp_u64
  - >> dwt_writetxfctrl
  - >> dwt_writetxdata
  - >> dwt_write32bitoffsetreg
  - >> dwt_starttx
  - >> dwt_setrxtimeout
  - >> dwt_setrxaftertxdelay
  - >> dwt_setdelayedtrxtime
  - >> dwt_rxenable
  - >> dwt_readrxdata
  - >> dwt_read32bitoffsetreg
  - >> GPIO_SetBits
  - >> final_msg_set_ts
  - >> distance_mange
  - >> memcmp
  [Called By]
  - >> TAG_MEASURE

  USART1_IRQHandler (Thumb, 36 bytes, Stack size 8 bytes, stm32_eval.o(i.USART1_IRQHandler))
  [Stack]

  - Max Depth = 1096
  - Call Chain = USART1_IRQHandler ⇒ at_cmd_recv ⇒ at_cmd_parse ⇒ __2printf
  [Calls]
  - >> USART_ReceiveData
  - >> USART_GetITStatus
  - >> at_cmd_recv
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  USART_ClearFlag (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_usart.o(i.USART_ClearFlag))
  [Called By]

  - >> fputc

  USART_Cmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_usart.o(i.USART_Cmd))
  [Called By]

  - >> STM_EVAL_COMInit

  USART_GetFlagStatus (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_usart.o(i.USART_GetFlagStatus))
  [Called By]

  - >> fputc

  USART_GetITStatus (Thumb, 62 bytes, Stack size 12 bytes, stm32f10x_usart.o(i.USART_GetITStatus))
  [Stack]

  - Max Depth = 12
  - Call Chain = USART_GetITStatus
  [Called By]
  - >> USART1_IRQHandler

  USART_ITConfig (Thumb, 48 bytes, Stack size 8 bytes, stm32f10x_usart.o(i.USART_ITConfig))
  [Stack]

  - Max Depth = 8
  - Call Chain = USART_ITConfig
  [Called By]
  - >> STM_EVAL_COMInit

  USART_Init (Thumb, 166 bytes, Stack size 32 bytes, stm32f10x_usart.o(i.USART_Init))
  [Stack]

  - Max Depth = 44
  - Call Chain = USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> RCC_GetClocksFreq
  [Called By]
  - >> STM_EVAL_COMInit

  USART_ReceiveData (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_usart.o(i.USART_ReceiveData))
  [Called By]

  - >> USART1_IRQHandler

  USART_SendData (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_usart.o(i.USART_SendData))
  [Called By]

  - >> fputc

  USART_puts (Thumb, 24 bytes, Stack size 16 bytes, port.o(i.USART_puts))
  [Stack]

  - Max Depth = 32
  - Call Chain = USART_puts ⇒ putchar ⇒ fputc
  [Calls]
  - >> putchar
  [Called By]
  - >> ANTHOR_MEASURE

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.UsageFault_Handler))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  __0printf (Thumb, 22 bytes, Stack size 24 bytes, printfa.o(i.__0printf), UNUSED)
  [Calls]

  - >> _printf_core

  __1printf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0printf), UNUSED)

  __2printf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0printf))
  [Stack]

  - Max Depth = 24
  - Call Chain = __2printf
  [Called By]
  - >> main
  - >> distance_mange
  - >> HardFault_Handler
  - >> drv_lis2dh12_get_angle
  - >> SHT20_read_tem
  - >> buo1Gpio
  - >> buo1DbGpio
  - >> at_cmd_parse
  - >> AT_CmdFunc_version
  - >> AT_CmdFunc_XYZ
  - >> AT_CmdFunc_TemHum
  - >> AT_CmdFunc_RST
  - >> AT_CmdFunc_ANCHOR_TAG

  __c89printf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0printf), UNUSED)

  printf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0printf))
  [Stack]

  - Max Depth = 24
  - Call Chain = printf
  [Called By]
  - >> SHT20_read_hum

  __0sprintf (Thumb, 34 bytes, Stack size 24 bytes, printfa.o(i.__0sprintf), UNUSED)
  [Calls]

  - >> _sputc
  - >> _printf_core

  __1sprintf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0sprintf), UNUSED)

  __2sprintf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0sprintf))
  [Stack]

  - Max Depth = 24
  - Call Chain = __2sprintf
  [Called By]
  - >> distance_mange

  __c89sprintf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0sprintf), UNUSED)

  sprintf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0sprintf), UNUSED)

  __ARM_fpclassify (Thumb, 40 bytes, Stack size 0 bytes, fpclassify.o(i.__ARM_fpclassify))
  [Called By]

  - >> pow
  - >> asin

  __aeabi_errno_addr (Thumb, 4 bytes, Stack size 0 bytes, errno.o(i.__aeabi_errno_addr))
  [Called By]

  - >> _strtoul
  - >> strtol
  - >> atoi

  __rt_errno_addr (Thumb, 0 bytes, Stack size 0 bytes, errno.o(i.__aeabi_errno_addr), UNUSED)

  __kernel_poly (Thumb, 170 bytes, Stack size 24 bytes, poly.o(i.__kernel_poly))
  [Stack]

  - Max Depth = 112
  - Call Chain = __kernel_poly ⇒ __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_dmul
  - >> __aeabi_dadd
  [Called By]
  - >> pow
  - >> asin

  __mathlib_dbl_divzero (Thumb, 12 bytes, Stack size 0 bytes, dunder.o(i.__mathlib_dbl_divzero))
  [Stack]

  - Max Depth = 40
  - Call Chain = __mathlib_dbl_divzero ⇒ __aeabi_ddiv ⇒ _double_round
  [Calls]
  - >> __aeabi_ddiv
  [Called By]
  - >> pow

  __mathlib_dbl_infnan (Thumb, 6 bytes, Stack size 0 bytes, dunder.o(i.__mathlib_dbl_infnan))
  [Stack]

  - Max Depth = 16
  - Call Chain = __mathlib_dbl_infnan ⇒ __ARM_scalbn
  [Calls]
  - >> __ARM_scalbn
  [Called By]
  - >> asin

  __mathlib_dbl_infnan2 (Thumb, 4 bytes, Stack size 0 bytes, dunder.o(i.__mathlib_dbl_infnan2))
  [Stack]

  - Max Depth = 88
  - Call Chain = __mathlib_dbl_infnan2 ⇒ __aeabi_dadd ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_dadd
  [Called By]
  - >> pow

  __mathlib_dbl_invalid (Thumb, 12 bytes, Stack size 0 bytes, dunder.o(i.__mathlib_dbl_invalid))
  [Stack]

  - Max Depth = 40
  - Call Chain = __mathlib_dbl_invalid ⇒ __aeabi_ddiv ⇒ _double_round
  [Calls]
  - >> __aeabi_ddiv
  [Called By]
  - >> pow
  - >> asin

  __mathlib_dbl_overflow (Thumb, 14 bytes, Stack size 0 bytes, dunder.o(i.__mathlib_dbl_overflow))
  [Stack]

  - Max Depth = 16
  - Call Chain = __mathlib_dbl_overflow ⇒ __ARM_scalbn
  [Calls]
  - >> __ARM_scalbn
  [Called By]
  - >> pow

  __mathlib_dbl_underflow (Thumb, 10 bytes, Stack size 0 bytes, dunder.o(i.__mathlib_dbl_underflow))
  [Stack]

  - Max Depth = 16
  - Call Chain = __mathlib_dbl_underflow ⇒ __ARM_scalbn
  [Calls]
  - >> __ARM_scalbn
  [Called By]
  - >> pow
  - >> asin

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  __set_errno (Thumb, 6 bytes, Stack size 0 bytes, errno.o(i.__set_errno))
  [Called By]

  - >> sqrt
  - >> pow
  - >> asin

  _dwt_configlde (Thumb, 48 bytes, Stack size 16 bytes, deca_device.o(i._dwt_configlde))
  [Stack]

  - Max Depth = 64
  - Call Chain = _dwt_configlde ⇒ dwt_write16bitoffsetreg ⇒ dwt_writetodevice ⇒ writetospi_serial ⇒ decamutexon
  [Calls]
  - >> dwt_writetodevice
  - >> dwt_write16bitoffsetreg
  [Called By]
  - >> dwt_configure

  _dwt_enableclocks (Thumb, 194 bytes, Stack size 16 bytes, deca_device.o(i._dwt_enableclocks))
  [Stack]

  - Max Depth = 72
  - Call Chain = _dwt_enableclocks ⇒ dwt_readfromdevice ⇒ readfromspi_serial ⇒ decamutexon
  [Calls]
  - >> dwt_writetodevice
  - >> dwt_readfromdevice
  [Called By]
  - >> dwt_initialise
  - >> _dwt_loaducodefromrom

  _dwt_loaducodefromrom (Thumb, 52 bytes, Stack size 8 bytes, deca_device.o(i._dwt_loaducodefromrom))
  [Stack]

  - Max Depth = 80
  - Call Chain = _dwt_loaducodefromrom ⇒ _dwt_enableclocks ⇒ dwt_readfromdevice ⇒ readfromspi_serial ⇒ decamutexon
  [Calls]
  - >> deca_sleep
  - >> dwt_writetodevice
  - >> dwt_write16bitoffsetreg
  - >> _dwt_enableclocks
  [Called By]
  - >> dwt_initialise

  _dwt_otpread (Thumb, 70 bytes, Stack size 8 bytes, deca_device.o(i._dwt_otpread))
  [Stack]

  - Max Depth = 80
  - Call Chain = _dwt_otpread ⇒ dwt_read32bitoffsetreg ⇒ dwt_readfromdevice ⇒ readfromspi_serial ⇒ decamutexon
  [Calls]
  - >> dwt_read32bitoffsetreg
  - >> dwt_writetodevice
  [Called By]
  - >> dwt_initialise

  asin (Thumb, 572 bytes, Stack size 56 bytes, asin.o(i.asin))
  [Stack]

  - Max Depth = 168
  - Call Chain = asin ⇒ __kernel_poly ⇒ __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_drsub
  - >> __aeabi_dsub
  - >> __aeabi_dmul
  - >> __aeabi_ddiv
  - >> __aeabi_dadd
  - >> __ARM_scalbn
  - >> sqrt
  - >> __set_errno
  - >> __kernel_poly
  - >> __ARM_fpclassify
  - >> __mathlib_dbl_underflow
  - >> __mathlib_dbl_invalid
  - >> __mathlib_dbl_infnan
  [Called By]
  - >> drv_lis2dh12_get_angle

  at_cmd_parse (Thumb, 214 bytes, Stack size 1040 bytes, stm32_eval.o(i.at_cmd_parse))
  [Stack]

  - Max Depth = 1064
  - Call Chain = at_cmd_parse ⇒ __2printf
  [Calls]
  - >> string_split
  - >> strlen
  - >> strstr
  - >> __aeabi_memclr4
  - >> __2printf
  [Called By]
  - >> at_cmd_recv

  at_cmd_recv (Thumb, 98 bytes, Stack size 24 bytes, stm32_eval.o(i.at_cmd_recv))
  [Stack]

  - Max Depth = 1088
  - Call Chain = at_cmd_recv ⇒ at_cmd_parse ⇒ __2printf
  [Calls]
  - >> portGetTickCnt
  - >> at_cmd_parse
  [Called By]
  - >> USART1_IRQHandler

  buo1DbGpio (Thumb, 214 bytes, Stack size 16 bytes, stm32_eval.o(i.buo1DbGpio))
  [Stack]

  - Max Depth = 76
  - Call Chain = buo1DbGpio ⇒ PairGpioCheckDB ⇒ GPIO_Init
  [Calls]
  - >> GPIO_PinRemapConfig
  - >> RCC_APB2PeriphClockCmd
  - >> PairGpioCheckDB
  - >> __2printf
  [Called By]
  - >> AT_CmdFunc_ANCHOR_GPIOTEST

  buo1Gpio (Thumb, 80 bytes, Stack size 8 bytes, stm32_eval.o(i.buo1Gpio))
  [Stack]

  - Max Depth = 112
  - Call Chain = buo1Gpio ⇒ PairGpioCheck ⇒ dwt_getgpiovalue ⇒ dwt_read32bitoffsetreg ⇒ dwt_readfromdevice ⇒ readfromspi_serial ⇒ decamutexon
  [Calls]
  - >> dwt_enablegpioclocks1
  - >> dwt_enablegpioclocks
  - >> PairGpioCheck
  - >> __2printf
  [Called By]
  - >> AT_CmdFunc_ANCHOR_GPIOTEST

  deca_sleep (Thumb, 24 bytes, Stack size 8 bytes, deca_sleep.o(i.deca_sleep))
  [Stack]

  - Max Depth = 8
  - Call Chain = deca_sleep
  [Calls]
  - >> portGetTickCnt
  [Called By]
  - >> reset_DW1000
  - >> peripherals_init
  - >> main
  - >> _dwt_loaducodefromrom

  decamutexoff (Thumb, 18 bytes, Stack size 0 bytes, deca_mutex.o(i.decamutexoff))
  [Called By]

  - >> writetospi_serial
  - >> readfromspi_serial
  - >> dwt_forcetrxoff

  decamutexon (Thumb, 26 bytes, Stack size 8 bytes, deca_mutex.o(i.decamutexon))
  [Stack]

  - Max Depth = 8
  - Call Chain = decamutexon
  [Calls]
  - >> EXTI_GetITEnStatus
  [Called By]
  - >> writetospi_serial
  - >> readfromspi_serial
  - >> dwt_forcetrxoff

  drv_lis2dh12_get_angle (Thumb, 332 bytes, Stack size 48 bytes, lcd_oled.o(i.drv_lis2dh12_get_angle))
  [Stack]

  - Max Depth = 272
  - Call Chain = drv_lis2dh12_get_angle ⇒ pow ⇒ __kernel_poly ⇒ __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_i2f
  - >> __aeabi_fdiv
  - >> __aeabi_f2d
  - >> __aeabi_fsub
  - >> __aeabi_f2iz
  - >> __aeabi_dmul
  - >> __aeabi_ddiv
  - >> __aeabi_dadd
  - >> __aeabi_d2f
  - >> __aeabi_cfrcmple
  - >> __ARM_scalbn
  - >> drv_lis2dh12_iic_read_byte
  - >> sqrt
  - >> pow
  - >> asin
  - >> __2printf
  [Called By]
  - >> AT_CmdFunc_XYZ

  drv_lis2dh12_iic_read_byte (Thumb, 230 bytes, Stack size 32 bytes, lcd_oled.o(i.drv_lis2dh12_iic_read_byte))
  [Stack]

  - Max Depth = 44
  - Call Chain = drv_lis2dh12_iic_read_byte ⇒ I2C_GetFlagStatus
  [Calls]
  - >> I2C_SendData
  - >> I2C_Send7bitAddress
  - >> I2C_ReceiveData
  - >> I2C_NACKPositionConfig
  - >> I2C_GetFlagStatus
  - >> I2C_GenerateSTOP
  - >> I2C_GenerateSTART
  - >> I2C_CheckEvent
  - >> I2C_AcknowledgeConfig
  [Called By]
  - >> drv_lis2dh12_get_angle

  drv_lis2dh12_iic_write_byte (Thumb, 18 bytes, Stack size 8 bytes, lcd_oled.o(i.drv_lis2dh12_iic_write_byte))
  [Stack]

  - Max Depth = 52
  - Call Chain = drv_lis2dh12_iic_write_byte ⇒ I2C_WriteOneByte ⇒ I2C_GetFlagStatus
  [Calls]
  - >> I2C_WriteOneByte
  [Called By]
  - >> drv_lis2dh12_init

  drv_lis2dh12_init (Thumb, 70 bytes, Stack size 8 bytes, lcd_oled.o(i.drv_lis2dh12_init))
  [Stack]

  - Max Depth = 60
  - Call Chain = drv_lis2dh12_init ⇒ drv_lis2dh12_iic_write_byte ⇒ I2C_WriteOneByte ⇒ I2C_GetFlagStatus
  [Calls]
  - >> drv_lis2dh12_iic_write_byte
  [Called By]
  - >> peripherals_init

  dwt_configure (Thumb, 490 bytes, Stack size 40 bytes, deca_device.o(i.dwt_configure))
  [Stack]

  - Max Depth = 104
  - Call Chain = dwt_configure ⇒ _dwt_configlde ⇒ dwt_write16bitoffsetreg ⇒ dwt_writetodevice ⇒ writetospi_serial ⇒ decamutexon
  [Calls]
  - >> dwt_write32bitoffsetreg
  - >> dwt_writetodevice
  - >> dwt_write16bitoffsetreg
  - >> _dwt_configlde
  [Called By]
  - >> main

  dwt_enablegpioclocks (Thumb, 26 bytes, Stack size 8 bytes, deca_device.o(i.dwt_enablegpioclocks))
  [Stack]

  - Max Depth = 80
  - Call Chain = dwt_enablegpioclocks ⇒ dwt_read32bitoffsetreg ⇒ dwt_readfromdevice ⇒ readfromspi_serial ⇒ decamutexon
  [Calls]
  - >> dwt_write32bitoffsetreg
  - >> dwt_read32bitoffsetreg
  [Called By]
  - >> buo1Gpio

  dwt_enablegpioclocks1 (Thumb, 44 bytes, Stack size 8 bytes, deca_device.o(i.dwt_enablegpioclocks1))
  [Stack]

  - Max Depth = 64
  - Call Chain = dwt_enablegpioclocks1 ⇒ dwt_readfromdevice ⇒ readfromspi_serial ⇒ decamutexon
  [Calls]
  - >> dwt_writetodevice
  - >> dwt_readfromdevice
  [Called By]
  - >> buo1Gpio

  dwt_entersleepaftertx (Thumb, 36 bytes, Stack size 8 bytes, deca_device.o(i.dwt_entersleepaftertx))
  [Stack]

  - Max Depth = 80
  - Call Chain = dwt_entersleepaftertx ⇒ dwt_read32bitoffsetreg ⇒ dwt_readfromdevice ⇒ readfromspi_serial ⇒ decamutexon
  [Calls]
  - >> dwt_write32bitoffsetreg
  - >> dwt_read32bitoffsetreg
  [Called By]
  - >> dwt_starttx

  dwt_forcetrxoff (Thumb, 86 bytes, Stack size 16 bytes, deca_device.o(i.dwt_forcetrxoff))
  [Stack]

  - Max Depth = 88
  - Call Chain = dwt_forcetrxoff ⇒ dwt_read32bitoffsetreg ⇒ dwt_readfromdevice ⇒ readfromspi_serial ⇒ decamutexon
  [Calls]
  - >> dwt_write32bitoffsetreg
  - >> dwt_read32bitoffsetreg
  - >> decamutexon
  - >> decamutexoff
  - >> dwt_writetodevice
  - >> dwt_syncrxbufptrs
  [Called By]
  - >> dwt_rxenable

  dwt_getgpiovalue (Thumb, 20 bytes, Stack size 8 bytes, deca_device.o(i.dwt_getgpiovalue))
  [Stack]

  - Max Depth = 80
  - Call Chain = dwt_getgpiovalue ⇒ dwt_read32bitoffsetreg ⇒ dwt_readfromdevice ⇒ readfromspi_serial ⇒ decamutexon
  [Calls]
  - >> dwt_read32bitoffsetreg
  [Called By]
  - >> PairGpioCheck

  dwt_getrangebias (Thumb, 200 bytes, Stack size 16 bytes, deca_range_tables.o(i.dwt_getrangebias))
  [Stack]

  - Max Depth = 104
  - Call Chain = dwt_getrangebias ⇒ __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_i2f
  - >> __aeabi_f2d
  - >> __aeabi_d2iz
  - >> __aeabi_dmul
  - >> __ARM_scalbn
  [Called By]
  - >> ANTHOR_MEASURE

  dwt_initialise (Thumb, 208 bytes, Stack size 24 bytes, deca_device.o(i.dwt_initialise))
  [Stack]

  - Max Depth = 104
  - Call Chain = dwt_initialise ⇒ _dwt_otpread ⇒ dwt_read32bitoffsetreg ⇒ dwt_readfromdevice ⇒ readfromspi_serial ⇒ decamutexon
  [Calls]
  - >> dwt_read32bitoffsetreg
  - >> dwt_xtaltrim
  - >> dwt_writetodevice
  - >> dwt_write16bitoffsetreg
  - >> dwt_readdevid
  - >> dwt_read16bitoffsetreg
  - >> _dwt_otpread
  - >> _dwt_loaducodefromrom
  - >> _dwt_enableclocks
  [Called By]
  - >> main

  dwt_read16bitoffsetreg (Thumb, 38 bytes, Stack size 16 bytes, deca_device.o(i.dwt_read16bitoffsetreg))
  [Stack]

  - Max Depth = 72
  - Call Chain = dwt_read16bitoffsetreg ⇒ dwt_readfromdevice ⇒ readfromspi_serial ⇒ decamutexon
  [Calls]
  - >> dwt_readfromdevice
  [Called By]
  - >> dwt_starttx
  - >> dwt_initialise

  dwt_read32bitoffsetreg (Thumb, 38 bytes, Stack size 16 bytes, deca_device.o(i.dwt_read32bitoffsetreg))
  [Stack]

  - Max Depth = 72
  - Call Chain = dwt_read32bitoffsetreg ⇒ dwt_readfromdevice ⇒ readfromspi_serial ⇒ decamutexon
  [Calls]
  - >> dwt_readfromdevice
  [Called By]
  - >> dwt_setrxaftertxdelay
  - >> dwt_initialise
  - >> TAG_MEASURE
  - >> ANTHOR_MEASURE
  - >> Tag_Measure_Dis
  - >> compute_angle_send_to_anthor0
  - >> dwt_getgpiovalue
  - >> dwt_enablegpioclocks
  - >> dwt_readdevid
  - >> dwt_forcetrxoff
  - >> dwt_entersleepaftertx
  - >> _dwt_otpread

  dwt_readdevid (Thumb, 8 bytes, Stack size 0 bytes, deca_device.o(i.dwt_readdevid))
  [Stack]

  - Max Depth = 72
  - Call Chain = dwt_readdevid ⇒ dwt_read32bitoffsetreg ⇒ dwt_readfromdevice ⇒ readfromspi_serial ⇒ decamutexon
  [Calls]
  - >> dwt_read32bitoffsetreg
  [Called By]
  - >> dwt_initialise

  dwt_readfromdevice (Thumb, 58 bytes, Stack size 8 bytes, deca_device.o(i.dwt_readfromdevice))
  [Stack]

  - Max Depth = 56
  - Call Chain = dwt_readfromdevice ⇒ readfromspi_serial ⇒ decamutexon
  [Calls]
  - >> readfromspi_serial
  [Called By]
  - >> dwt_setrxtimeout
  - >> dwt_setleds
  - >> dwt_rxenable
  - >> dwt_readrxdata
  - >> dwt_read32bitoffsetreg
  - >> dwt_enablegpioclocks1
  - >> dwt_xtaltrim
  - >> dwt_syncrxbufptrs
  - >> dwt_readtxtimestamp
  - >> dwt_readrxtimestamp
  - >> dwt_read16bitoffsetreg
  - >> _dwt_enableclocks

  dwt_readrxdata (Thumb, 18 bytes, Stack size 8 bytes, deca_device.o(i.dwt_readrxdata))
  [Stack]

  - Max Depth = 64
  - Call Chain = dwt_readrxdata ⇒ dwt_readfromdevice ⇒ readfromspi_serial ⇒ decamutexon
  [Calls]
  - >> dwt_readfromdevice
  [Called By]
  - >> TAG_MEASURE
  - >> ANTHOR_MEASURE
  - >> Tag_Measure_Dis

  dwt_readrxtimestamp (Thumb, 12 bytes, Stack size 0 bytes, deca_device.o(i.dwt_readrxtimestamp))
  [Stack]

  - Max Depth = 56
  - Call Chain = dwt_readrxtimestamp ⇒ dwt_readfromdevice ⇒ readfromspi_serial ⇒ decamutexon
  [Calls]
  - >> dwt_readfromdevice
  [Called By]
  - >> get_rx_timestamp_u64

  dwt_readtxtimestamp (Thumb, 12 bytes, Stack size 0 bytes, deca_device.o(i.dwt_readtxtimestamp))
  [Stack]

  - Max Depth = 56
  - Call Chain = dwt_readtxtimestamp ⇒ dwt_readfromdevice ⇒ readfromspi_serial ⇒ decamutexon
  [Calls]
  - >> dwt_readfromdevice
  [Called By]
  - >> get_tx_timestamp_u64

  dwt_rxenable (Thumb, 80 bytes, Stack size 16 bytes, deca_device.o(i.dwt_rxenable))
  [Stack]

  - Max Depth = 104
  - Call Chain = dwt_rxenable ⇒ dwt_forcetrxoff ⇒ dwt_read32bitoffsetreg ⇒ dwt_readfromdevice ⇒ readfromspi_serial ⇒ decamutexon
  [Calls]
  - >> dwt_write16bitoffsetreg
  - >> dwt_syncrxbufptrs
  - >> dwt_readfromdevice
  - >> dwt_forcetrxoff
  [Called By]
  - >> TAG_MEASURE
  - >> ANTHOR_MEASURE
  - >> Tag_Measure_Dis

  dwt_setGPIOdirection (Thumb, 34 bytes, Stack size 8 bytes, deca_device.o(i.dwt_setGPIOdirection))
  [Stack]

  - Max Depth = 48
  - Call Chain = dwt_setGPIOdirection ⇒ dwt_writetodevice ⇒ writetospi_serial ⇒ decamutexon
  [Calls]
  - >> dwt_writetodevice
  [Called By]
  - >> PairGpioCheck

  dwt_setGPIOvalue (Thumb, 34 bytes, Stack size 8 bytes, deca_device.o(i.dwt_setGPIOvalue))
  [Stack]

  - Max Depth = 48
  - Call Chain = dwt_setGPIOvalue ⇒ dwt_writetodevice ⇒ writetospi_serial ⇒ decamutexon
  [Calls]
  - >> dwt_writetodevice
  [Called By]
  - >> PairGpioCheck

  dwt_setdelayedtrxtime (Thumb, 10 bytes, Stack size 0 bytes, deca_device.o(i.dwt_setdelayedtrxtime))
  [Stack]

  - Max Depth = 56
  - Call Chain = dwt_setdelayedtrxtime ⇒ dwt_write32bitoffsetreg ⇒ dwt_writetodevice ⇒ writetospi_serial ⇒ decamutexon
  [Calls]
  - >> dwt_write32bitoffsetreg
  [Called By]
  - >> Tag_Measure_Dis

  dwt_setleds (Thumb, 184 bytes, Stack size 16 bytes, deca_device.o(i.dwt_setleds))
  [Stack]

  - Max Depth = 72
  - Call Chain = dwt_setleds ⇒ dwt_readfromdevice ⇒ readfromspi_serial ⇒ decamutexon
  [Calls]
  - >> dwt_writetodevice
  - >> dwt_readfromdevice
  [Called By]
  - >> main

  dwt_setrxaftertxdelay (Thumb, 34 bytes, Stack size 8 bytes, deca_device.o(i.dwt_setrxaftertxdelay))
  [Stack]

  - Max Depth = 80
  - Call Chain = dwt_setrxaftertxdelay ⇒ dwt_read32bitoffsetreg ⇒ dwt_readfromdevice ⇒ readfromspi_serial ⇒ decamutexon
  [Calls]
  - >> dwt_write32bitoffsetreg
  - >> dwt_read32bitoffsetreg
  [Called By]
  - >> TAG_MEASURE
  - >> ANTHOR_MEASURE
  - >> main
  - >> Tag_Measure_Dis

  dwt_setrxantennadelay (Thumb, 12 bytes, Stack size 0 bytes, deca_device.o(i.dwt_setrxantennadelay))
  [Stack]

  - Max Depth = 48
  - Call Chain = dwt_setrxantennadelay ⇒ dwt_write16bitoffsetreg ⇒ dwt_writetodevice ⇒ writetospi_serial ⇒ decamutexon
  [Calls]
  - >> dwt_write16bitoffsetreg
  [Called By]
  - >> main

  dwt_setrxtimeout (Thumb, 84 bytes, Stack size 16 bytes, deca_device.o(i.dwt_setrxtimeout))
  [Stack]

  - Max Depth = 72
  - Call Chain = dwt_setrxtimeout ⇒ dwt_readfromdevice ⇒ readfromspi_serial ⇒ decamutexon
  [Calls]
  - >> dwt_writetodevice
  - >> dwt_write16bitoffsetreg
  - >> dwt_readfromdevice
  [Called By]
  - >> TAG_MEASURE
  - >> ANTHOR_MEASURE
  - >> main
  - >> Tag_Measure_Dis

  dwt_settxantennadelay (Thumb, 10 bytes, Stack size 0 bytes, deca_device.o(i.dwt_settxantennadelay))
  [Stack]

  - Max Depth = 48
  - Call Chain = dwt_settxantennadelay ⇒ dwt_write16bitoffsetreg ⇒ dwt_writetodevice ⇒ writetospi_serial ⇒ decamutexon
  [Calls]
  - >> dwt_write16bitoffsetreg
  [Called By]
  - >> main

  dwt_starttx (Thumb, 142 bytes, Stack size 24 bytes, deca_device.o(i.dwt_starttx))
  [Stack]

  - Max Depth = 104
  - Call Chain = dwt_starttx ⇒ dwt_entersleepaftertx ⇒ dwt_read32bitoffsetreg ⇒ dwt_readfromdevice ⇒ readfromspi_serial ⇒ decamutexon
  [Calls]
  - >> dwt_writetodevice
  - >> dwt_read16bitoffsetreg
  - >> dwt_entersleepaftertx
  [Called By]
  - >> TAG_MEASURE
  - >> ANTHOR_MEASURE
  - >> Tag_Measure_Dis
  - >> compute_angle_send_to_anthor0

  dwt_syncrxbufptrs (Thumb, 52 bytes, Stack size 16 bytes, deca_device.o(i.dwt_syncrxbufptrs))
  [Stack]

  - Max Depth = 72
  - Call Chain = dwt_syncrxbufptrs ⇒ dwt_readfromdevice ⇒ readfromspi_serial ⇒ decamutexon
  [Calls]
  - >> dwt_writetodevice
  - >> dwt_readfromdevice
  [Called By]
  - >> dwt_rxenable
  - >> dwt_forcetrxoff

  dwt_write16bitoffsetreg (Thumb, 26 bytes, Stack size 8 bytes, deca_device.o(i.dwt_write16bitoffsetreg))
  [Stack]

  - Max Depth = 48
  - Call Chain = dwt_write16bitoffsetreg ⇒ dwt_writetodevice ⇒ writetospi_serial ⇒ decamutexon
  [Calls]
  - >> dwt_writetodevice
  [Called By]
  - >> dwt_settxantennadelay
  - >> dwt_setrxtimeout
  - >> dwt_setrxantennadelay
  - >> dwt_rxenable
  - >> dwt_initialise
  - >> dwt_configure
  - >> _dwt_loaducodefromrom
  - >> _dwt_configlde

  dwt_write32bitoffsetreg (Thumb, 30 bytes, Stack size 16 bytes, deca_device.o(i.dwt_write32bitoffsetreg))
  [Stack]

  - Max Depth = 56
  - Call Chain = dwt_write32bitoffsetreg ⇒ dwt_writetodevice ⇒ writetospi_serial ⇒ decamutexon
  [Calls]
  - >> dwt_writetodevice
  [Called By]
  - >> dwt_writetxfctrl
  - >> dwt_setrxaftertxdelay
  - >> dwt_setdelayedtrxtime
  - >> dwt_configure
  - >> TAG_MEASURE
  - >> ANTHOR_MEASURE
  - >> Tag_Measure_Dis
  - >> dwt_enablegpioclocks
  - >> dwt_forcetrxoff
  - >> dwt_entersleepaftertx

  dwt_writetodevice (Thumb, 62 bytes, Stack size 8 bytes, deca_device.o(i.dwt_writetodevice))
  [Stack]

  - Max Depth = 40
  - Call Chain = dwt_writetodevice ⇒ writetospi_serial ⇒ decamutexon
  [Calls]
  - >> writetospi_serial
  [Called By]
  - >> dwt_writetxdata
  - >> dwt_write32bitoffsetreg
  - >> dwt_starttx
  - >> dwt_setrxtimeout
  - >> dwt_setleds
  - >> dwt_initialise
  - >> dwt_configure
  - >> dwt_setGPIOvalue
  - >> dwt_setGPIOdirection
  - >> dwt_enablegpioclocks1
  - >> dwt_xtaltrim
  - >> dwt_write16bitoffsetreg
  - >> dwt_syncrxbufptrs
  - >> dwt_forcetrxoff
  - >> _dwt_otpread
  - >> _dwt_loaducodefromrom
  - >> _dwt_enableclocks
  - >> _dwt_configlde

  dwt_writetxdata (Thumb, 34 bytes, Stack size 8 bytes, deca_device.o(i.dwt_writetxdata))
  [Stack]

  - Max Depth = 48
  - Call Chain = dwt_writetxdata ⇒ dwt_writetodevice ⇒ writetospi_serial ⇒ decamutexon
  [Calls]
  - >> dwt_writetodevice
  [Called By]
  - >> TAG_MEASURE
  - >> ANTHOR_MEASURE
  - >> Tag_Measure_Dis
  - >> compute_angle_send_to_anthor0

  dwt_writetxfctrl (Thumb, 24 bytes, Stack size 8 bytes, deca_device.o(i.dwt_writetxfctrl))
  [Stack]

  - Max Depth = 64
  - Call Chain = dwt_writetxfctrl ⇒ dwt_write32bitoffsetreg ⇒ dwt_writetodevice ⇒ writetospi_serial ⇒ decamutexon
  [Calls]
  - >> dwt_write32bitoffsetreg
  [Called By]
  - >> TAG_MEASURE
  - >> ANTHOR_MEASURE
  - >> Tag_Measure_Dis
  - >> compute_angle_send_to_anthor0

  dwt_xtaltrim (Thumb, 48 bytes, Stack size 16 bytes, deca_device.o(i.dwt_xtaltrim))
  [Stack]

  - Max Depth = 72
  - Call Chain = dwt_xtaltrim ⇒ dwt_readfromdevice ⇒ readfromspi_serial ⇒ decamutexon
  [Calls]
  - >> dwt_writetodevice
  - >> dwt_readfromdevice
  [Called By]
  - >> dwt_initialise

  filter (Thumb, 84 bytes, Stack size 20 bytes, main.o(i.filter))
  [Stack]

  - Max Depth = 20
  - Call Chain = filter
  [Called By]
  - >> distance_mange

  fputc (Thumb, 38 bytes, Stack size 16 bytes, main.o(i.fputc))
  [Stack]

  - Max Depth = 16
  - Call Chain = fputc
  [Calls]
  - >> USART_SendData
  - >> USART_GetFlagStatus
  - >> USART_ClearFlag
  [Called By]
  - >> putchar
  - >> putc
  [Address Reference Count : 1]
  - printfa.o(i.__0printf)

  get_rx_timestamp_u64 (Thumb, 38 bytes, Stack size 24 bytes, lib.o(i.get_rx_timestamp_u64))
  [Stack]

  - Max Depth = 80
  - Call Chain = get_rx_timestamp_u64 ⇒ dwt_readrxtimestamp ⇒ dwt_readfromdevice ⇒ readfromspi_serial ⇒ decamutexon
  [Calls]
  - >> dwt_readrxtimestamp
  [Called By]
  - >> ANTHOR_MEASURE
  - >> Tag_Measure_Dis

  get_tx_timestamp_u64 (Thumb, 38 bytes, Stack size 24 bytes, lib.o(i.get_tx_timestamp_u64))
  [Stack]

  - Max Depth = 80
  - Call Chain = get_tx_timestamp_u64 ⇒ dwt_readtxtimestamp ⇒ dwt_readfromdevice ⇒ readfromspi_serial ⇒ decamutexon
  [Calls]
  - >> dwt_readtxtimestamp
  [Called By]
  - >> ANTHOR_MEASURE
  - >> Tag_Measure_Dis

  hal_i2c1_read_data (Thumb, 322 bytes, Stack size 56 bytes, lcd_oled.o(i.hal_i2c1_read_data))
  [Stack]

  - Max Depth = 68
  - Call Chain = hal_i2c1_read_data ⇒ I2C_GetFlagStatus
  [Calls]
  - >> I2C_Send7bitAddress
  - >> I2C_ReceiveData
  - >> I2C_NACKPositionConfig
  - >> I2C_GetFlagStatus
  - >> I2C_GenerateSTOP
  - >> I2C_GenerateSTART
  - >> I2C_CheckEvent
  - >> I2C_AcknowledgeConfig
  [Called By]
  - >> SHT20_read_tem
  - >> SHT20_read_hum
  - >> SHT20_init

  hal_i2c1_send_data (Thumb, 50 bytes, Stack size 32 bytes, lcd_oled.o(i.hal_i2c1_send_data))
  [Stack]

  - Max Depth = 68
  - Call Chain = hal_i2c1_send_data ⇒ hal_i2c1_send_data1 ⇒ I2C_GetFlagStatus
  [Calls]
  - >> hal_i2c1_send_data1
  [Called By]
  - >> SHT20_read_tem
  - >> SHT20_read_hum
  - >> SHT20_init

  hal_i2c1_send_data1 (Thumb, 156 bytes, Stack size 24 bytes, lcd_oled.o(i.hal_i2c1_send_data1))
  [Stack]

  - Max Depth = 36
  - Call Chain = hal_i2c1_send_data1 ⇒ I2C_GetFlagStatus
  [Calls]
  - >> I2C_SendData
  - >> I2C_Send7bitAddress
  - >> I2C_GetFlagStatus
  - >> I2C_GenerateSTOP
  - >> I2C_GenerateSTART
  - >> I2C_CheckEvent
  - >> I2C_AcknowledgeConfig
  [Called By]
  - >> hal_i2c1_send_data

  main (Thumb, 358 bytes, Stack size 24 bytes, main.o(i.main))
  [Stack]

  - Max Depth = 224
  - Call Chain = main ⇒ TAG_MEASURE ⇒ Tag_Measure_Dis ⇒ distance_mange ⇒ compute_angle_send_to_anthor0 ⇒ dwt_starttx ⇒ dwt_entersleepaftertx ⇒ dwt_read32bitoffsetreg ⇒ dwt_readfromdevice ⇒ readfromspi_serial ⇒ decamutexon
  [Calls]
  - >> spi_set_rate_low
  - >> spi_set_rate_high
  - >> reset_DW1000
  - >> peripherals_init
  - >> dwt_settxantennadelay
  - >> dwt_setrxtimeout
  - >> dwt_setrxantennadelay
  - >> dwt_setrxaftertxdelay
  - >> dwt_setleds
  - >> dwt_initialise
  - >> dwt_configure
  - >> deca_sleep
  - >> TAG_MEASURE
  - >> OLED_ShowString
  - >> GPIO_SetBits
  - >> GPIO_ResetBits
  - >> FLASH_ReadMoreData
  - >> ANTHOR_MEASURE
  - >> Semaphore_Init
  - >> Anchor_Array_Init
  - >> __2printf
  [Address Reference Count : 1]
  - entry9a.o(.ARM.Collect$$$$0000000B)

  peripherals_init (Thumb, 72 bytes, Stack size 8 bytes, port.o(i.peripherals_init))
  [Stack]

  - Max Depth = 100
  - Call Chain = peripherals_init ⇒ SHT20_init ⇒ hal_i2c1_send_data ⇒ hal_i2c1_send_data1 ⇒ I2C_GetFlagStatus
  [Calls]
  - >> RCC_APB2PeriphClockCmd
  - >> RCC_APB1PeriphClockCmd
  - >> deca_sleep
  - >> drv_lis2dh12_init
  - >> SHT20_init
  - >> OLED_Init
  - >> OLED_Clear
  - >> usartinit
  - >> SysTick_Configuration
  - >> SPI_Configuration
  - >> GPIO_Configuration
  - >> MX_I2C1_Init
  [Called By]
  - >> main

  portGetTickCnt (Thumb, 6 bytes, Stack size 0 bytes, port.o(i.portGetTickCnt))
  [Called By]

  - >> deca_sleep
  - >> TAG_MEASURE
  - >> Tag_Measure_Dis
  - >> at_cmd_recv

  pow (Thumb, 2478 bytes, Stack size 112 bytes, pow.o(i.pow))
  [Stack]

  - Max Depth = 224
  - Call Chain = pow ⇒ __kernel_poly ⇒ __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_i2d
  - >> __aeabi_cdrcmple
  - >> __aeabi_drsub
  - >> __aeabi_dsub
  - >> __aeabi_dmul
  - >> __aeabi_ddiv
  - >> __aeabi_dadd
  - >> __ARM_scalbn
  - >> sqrt
  - >> __set_errno
  - >> __kernel_poly
  - >> __ARM_fpclassify
  - >> __mathlib_dbl_underflow
  - >> __mathlib_dbl_overflow
  - >> __mathlib_dbl_invalid
  - >> __mathlib_dbl_infnan2
  - >> __mathlib_dbl_divzero
  [Called By]
  - >> drv_lis2dh12_get_angle

  putc (Thumb, 4 bytes, Stack size 0 bytes, putc.o(i.putc))
  [Stack]

  - Max Depth = 16
  - Call Chain = putc ⇒ fputc
  [Calls]
  - >> fputc
  [Called By]
  - >> ANTHOR_MEASURE

  putchar (Thumb, 6 bytes, Stack size 0 bytes, putchar.o(i.putchar))
  [Stack]

  - Max Depth = 16
  - Call Chain = putchar ⇒ fputc
  [Calls]
  - >> fputc
  [Called By]
  - >> USART_puts

  readfromspi_serial (Thumb, 114 bytes, Stack size 40 bytes, deca_spi.o(i.readfromspi_serial))
  [Stack]

  - Max Depth = 48
  - Call Chain = readfromspi_serial ⇒ decamutexon
  [Calls]
  - >> SPI_I2S_GetFlagStatus
  - >> decamutexon
  - >> decamutexoff
  [Called By]
  - >> dwt_readfromdevice

  reset_DW1000 (Thumb, 70 bytes, Stack size 24 bytes, port.o(i.reset_DW1000))
  [Stack]

  - Max Depth = 44
  - Call Chain = reset_DW1000 ⇒ GPIO_Init
  [Calls]
  - >> GPIO_Init
  - >> deca_sleep
  - >> GPIO_ResetBits
  [Called By]
  - >> main

  spi_set_rate_high (Thumb, 6 bytes, Stack size 0 bytes, port.o(i.spi_set_rate_high))
  [Calls]

  - >> SPI_ChangeRate
  [Called By]
  - >> main

  spi_set_rate_low (Thumb, 6 bytes, Stack size 0 bytes, port.o(i.spi_set_rate_low))
  [Calls]

  - >> SPI_ChangeRate
  [Called By]
  - >> main

  sqrt (Thumb, 76 bytes, Stack size 24 bytes, sqrt.o(i.sqrt))
  [Stack]

  - Max Depth = 64
  - Call Chain = sqrt ⇒ _dsqrt ⇒ _double_round
  [Calls]
  - >> _dsqrt
  - >> __set_errno
  [Called By]
  - >> drv_lis2dh12_get_angle
  - >> pow
  - >> asin

  string_split (Thumb, 28 bytes, Stack size 8 bytes, stm32_eval.o(i.string_split))
  [Stack]

  - Max Depth = 8
  - Call Chain = string_split
  [Called By]
  - >> at_cmd_parse

  usartinit (Thumb, 42 bytes, Stack size 24 bytes, port.o(i.usartinit))
  [Stack]

  - Max Depth = 92
  - Call Chain = usartinit ⇒ STM_EVAL_COMInit ⇒ USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> STM_EVAL_COMInit
  [Called By]
  - >> peripherals_init

  writetospi_serial (Thumb, 90 bytes, Stack size 24 bytes, deca_spi.o(i.writetospi_serial))
  [Stack]

  - Max Depth = 32
  - Call Chain = writetospi_serial ⇒ decamutexon
  [Calls]
  - >> decamutexon
  - >> decamutexoff
  [Called By]
  - >> dwt_writetodevice

  ### Local Symbols

  compute_angle_send_to_anthor0 (Thumb, 186 bytes, Stack size 24 bytes, main.o(i.compute_angle_send_to_anthor0))
  [Stack]

  - Max Depth = 128
  - Call Chain = compute_angle_send_to_anthor0 ⇒ dwt_starttx ⇒ dwt_entersleepaftertx ⇒ dwt_read32bitoffsetreg ⇒ dwt_readfromdevice ⇒ readfromspi_serial ⇒ decamutexon
  [Calls]
  - >> dwt_writetxfctrl
  - >> dwt_writetxdata
  - >> dwt_starttx
  - >> dwt_read32bitoffsetreg
  [Called By]
  - >> distance_mange

  distance_mange (Thumb, 282 bytes, Stack size 32 bytes, main.o(i.distance_mange))
  [Stack]

  - Max Depth = 160
  - Call Chain = distance_mange ⇒ compute_angle_send_to_anthor0 ⇒ dwt_starttx ⇒ dwt_entersleepaftertx ⇒ dwt_read32bitoffsetreg ⇒ dwt_readfromdevice ⇒ readfromspi_serial ⇒ decamutexon
  [Calls]
  - >> __aeabi_i2f
  - >> __aeabi_fdiv
  - >> __aeabi_f2d
  - >> OLED_ShowString
  - >> filter
  - >> compute_angle_send_to_anthor0
  - >> __2sprintf
  - >> __2printf
  [Called By]
  - >> Tag_Measure_Dis

  final_msg_set_ts (Thumb, 22 bytes, Stack size 8 bytes, main.o(i.final_msg_set_ts))
  [Stack]

  - Max Depth = 8
  - Call Chain = final_msg_set_ts
  [Called By]
  - >> Tag_Measure_Dis

  SetSysClockTo72 (Thumb, 160 bytes, Stack size 12 bytes, system_stm32f10x.o(i.SetSysClockTo72))
  [Stack]

  - Max Depth = 12
  - Call Chain = SetSysClockTo72
  [Called By]
  - >> SystemInit

  MX_I2C1_Init (Thumb, 106 bytes, Stack size 16 bytes, port.o(i.MX_I2C1_Init))
  [Stack]

  - Max Depth = 68
  - Call Chain = MX_I2C1_Init ⇒ I2C_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> GPIO_Init
  - >> RCC_APB2PeriphClockCmd
  - >> RCC_APB1PeriphClockCmd
  - >> I2C_Init
  - >> I2C_DeInit
  - >> I2C_Cmd
  - >> I2C_AcknowledgeConfig
  [Called By]
  - >> peripherals_init

  NVIC_SetPriority (Thumb, 32 bytes, Stack size 0 bytes, port.o(i.NVIC_SetPriority))
  [Called By]

  - >> SysTick_Configuration

  NVIC_SystemReset (Thumb, 20 bytes, Stack size 0 bytes, lib.o(i.NVIC_SystemReset))
  [Called By]

  - >> TAG_MEASURE

  final_msg_get_ts (Thumb, 26 bytes, Stack size 8 bytes, lib.o(i.final_msg_get_ts))
  [Stack]

  - Max Depth = 8
  - Call Chain = final_msg_get_ts
  [Called By]
  - >> ANTHOR_MEASURE

  _fp_digits (Thumb, 334 bytes, Stack size 56 bytes, printfa.o(i._fp_digits), UNUSED)
  [Calls]

  - >> __aeabi_cdrcmple
  - >> __aeabi_dmul
  - >> __aeabi_ddiv
  - >> __aeabi_dadd
  - >> __aeabi_uldivmod
  - >> __aeabi_d2ulz
  [Called By]
  - >> _printf_core

  _printf_core (Thumb, 1744 bytes, Stack size 136 bytes, printfa.o(i._printf_core), UNUSED)
  [Calls]

  - >> __aeabi_uldivmod
  - >> __aeabi_uidivmod
  - >> _printf_pre_padding
  - >> _printf_post_padding
  - >> _fp_digits
  [Called By]
  - >> __0sprintf
  - >> __0printf

  _printf_post_padding (Thumb, 36 bytes, Stack size 24 bytes, printfa.o(i._printf_post_padding), UNUSED)
  [Called By]

  - >> _printf_core

  _printf_pre_padding (Thumb, 46 bytes, Stack size 24 bytes, printfa.o(i._printf_pre_padding), UNUSED)
  [Called By]

  - >> _printf_core

  _sputc (Thumb, 10 bytes, Stack size 0 bytes, printfa.o(i._sputc))
  [Called By]

  - >> __0sprintf
  [Address Reference Count : 1]
  - printfa.o(i.__0sprintf)

  ### Undefined Global Symbols